WB32F10x Standard Peripherals Firmware Library

成员变量
TIM_BDTRInitTypeDef结构体 参考
WB32F10x_StdPeriph_Driver » TIM

BDTR structure definition 更多...

`#include <wb32f10x_tim.h>`

## 成员变量
uint16_t | TIM_OSSRState
uint16_t | TIM_OSSIState
uint16_t | TIM_LOCKLevel
uint16_t | TIM_DeadTime
uint16_t | TIM_Break
uint16_t | TIM_BreakPolarity
uint16_t | TIM_AutomaticOutput

## 详细描述

BDTR structure definition

注解
  This structure is used only with TIM1.

## 结构体成员变量说明

## ◆ TIM_AutomaticOutput

uint16_t TIM_AutomaticOutput

Specifies whether the TIM Automatic Output feature is enabled or not. This parameter can be a value of TIM_AOE_Bit_Set_Reset

## ◆ TIM_Break

uint16_t TIM_Break

Specifies whether the TIM Break input is enabled or not. This parameter can be a value of Break_Input_enable_disable

## ◆ TIM_BreakPolarity

uint16_t TIM_BreakPolarity

Specifies the TIM Break Input pin polarity. This parameter can be a value of Break_Polarity

## ◆ TIM_DeadTime

uint16_t TIM_DeadTime

Specifies the delay time between the switching-off and the switching-on of the outputs. This parameter can be a number between 0x00 and 0xFF

## ◆ TIM_LOCKLevel

uint16_t TIM_LOCKLevel

Specifies the LOCK level parameters. This parameter can be a value of Lock_level

## ◆ TIM_OSSIState

uint16_t TIM_OSSIState

Specifies the Off-State used in Idle state. This parameter can be a value of OSSI_Off_State_Selection_for_Idle_mode_state

## ◆ TIM_OSSRState

uint16_t TIM_OSSRState

Specifies the Off-State selection used in Run mode. This parameter can be a value of OSSR_Off_State_Selection_for_Run_mode_state

该结构体的文档由以下文件生成:

- wb32f10x_tim.h