WB32F10x Standard Peripherals Firmware Library

Macros
RTC_output_source_to_output_on_the_Tamper_pin
WB32F10x_StdPeriph_Driver » BKP » BKP_Exported_Constants

## Macros
#define | BKP_RTCOutputSource_None ((uint16_t)0x0000)
#define | BKP_RTCOutputSource_CalibClock ((uint16_t)0x0080)
#define | BKP_RTCOutputSource_Alarm ((uint16_t)0x0100)
#define | BKP_RTCOutputSource_Second ((uint16_t)0x0300)
#define | IS_BKP_RTC_OUTPUT_SOURCE(SOURCE)

## Detailed Description

## Macro Definition Documentation

## ◆ IS_BKP_RTC_OUTPUT_SOURCE

#define IS_BKP_RTC_OUTPUT_SOURCE | ( |  | SOURCE | ) |

Value:
(((SOURCE) == BKP_RTCOutputSource_None) || \
((SOURCE) == BKP_RTCOutputSource_CalibClock) || \
((SOURCE) == BKP_RTCOutputSource_Alarm) || \
((SOURCE) == BKP_RTCOutputSource_Second))