WB32F10x Standard Peripherals Firmware Library

Enumerations | Functions
usbd_intr.c File Reference
`#include "wb32f10x.h"`
`#include <stdlib.h>`
`#include "usbd_core.h"`
`#include "usbd_user.h"`

## Enumerations
enum | Endpoint0State_t { EP0_STATE_IDLE, EP0_STATE_TX, EP0_STATE_RX, EP0_STATE_STALL }

## Functions
void | USBD_EndPoint0 (void)
| Handle Endpoint 0 Event. More...
void | Handle_USBD_INT (uint8_t IntrUSB, uint8_t IntrIn, uint8_t IntrOut)
| Handle USBD Interrupts. More...

## Detailed Description

Author
  Westberry Application Team

Attention

Copyright (c) 2020 - 2023 Westberry Technology (ChangZhou) Corp., Ltd All rights reserved.

THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME. AS A RESULT, WESTBERRY TECHNOLOGY SHALL NOT BE HELD LIABLE FOR ANY DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.

## Function Documentation

## ◆ Handle_USBD_INT()

void Handle_USBD_INT | ( | uint8_t | IntrUSB,
|  | uint8_t | IntrIn,
|  | uint8_t | IntrOut
| ) |  |

Handle USBD Interrupts.

Returns
  None

## ◆ USBD_EndPoint0()

void USBD_EndPoint0 | ( | void |  | ) |

Handle Endpoint 0 Event.

Returns
  None