WB32F10x Standard Peripherals Firmware Library

Modules | Macros
TIM_Exported_Constants
WB32F10x_StdPeriph_Driver » TIM

## Modules
| TIM_Output_Compare_and_PWM_modes
| TIM_One_Pulse_Mode
| TIM_Channel
| TIM_Clock_Division_CKD
| TIM_Counter_Mode
| TIM_Output_Compare_Polarity
| TIM_Output_Compare_N_Polarity
| TIM_Output_Compare_state
| TIM_Output_Compare_N_state
| TIM_Capture_Compare_state
| TIM_Capture_Compare_N_state
| Break_Input_enable_disable
| Break_Polarity
| TIM_AOE_Bit_Set_Reset
| Lock_level
| OSSI_Off_State_Selection_for_Idle_mode_state
| OSSR_Off_State_Selection_for_Run_mode_state
| TIM_Output_Compare_Idle_State
| TIM_Output_Compare_N_Idle_State
| TIM_Input_Capture_Polarity
| TIM_Input_Capture_Selection
| TIM_Input_Capture_Prescaler
| TIM_interrupt_sources
| TIM_DMA_sources
| TIM_External_Trigger_Prescaler
| TIM_Internal_Trigger_Selection
| TIM_TIx_External_Clock_Source
| TIM_External_Trigger_Polarity
| TIM_Prescaler_Reload_Mode
| TIM_Forced_Action
| TIM_Encoder_Mode
| TIM_Event_Source
| TIM_Update_Source
| TIM_Output_Compare_Preload_State
| TIM_Output_Compare_Fast_State
| TIM_Output_Compare_Clear_State
| TIM_Trigger_Output_Source
| TIM_Slave_Mode
| TIM_Master_Slave_Mode
| TIM_Flags
| TIM_Input_Capture_Filer_Value
| TIM_External_Trigger_Filter

## Macros
#define | IS_TIM_ALL_PERIPH(PERIPH)
#define | IS_TIM_LIST1_PERIPH(PERIPH) ((PERIPH) == TIM1)

## Detailed Description

## Macro Definition Documentation

## ◆ IS_TIM_ALL_PERIPH

#define IS_TIM_ALL_PERIPH | ( |  | PERIPH | ) |

Value:
(((PERIPH) == TIM1) || \
((PERIPH) == TIM2) || \
((PERIPH) == TIM3) || \
((PERIPH) == TIM4))