WB32F10x Standard Peripherals Firmware Library

成员变量
SPI_TypeDef结构体 参考
CMSIS » Wb32f10x

## 成员变量
__IOM uint32_t | CR0
__IOM uint32_t | CR1
__IOM uint32_t | SPIENR
__IOM uint32_t | MWCR
__IOM uint32_t | SER
__IOM uint32_t | BAUDR
__IOM uint32_t | TXFTLR
__IOM uint32_t | RXFTLR
__IM uint32_t | TXFLR
__IM uint32_t | RXFLR
__IM uint32_t | SR
__IOM uint32_t | IER
__IM uint32_t | ISR
__IM uint32_t | RISR
__IM uint32_t | TXOICR
__IM uint32_t | RXOICR
__IM uint32_t | RXUICR
__IM uint32_t | MSTICR
__IM uint32_t | ICR
__IOM uint32_t | DMACR
__IOM uint32_t | DMATDLR
__IOM uint32_t | DMARDLR
uint32_t | RESERVED0 [2]
__IOM uint32_t | DR
uint32_t | RESERVED1 [35]
__IOM uint32_t | RX_SAMPLE_DLY
__IOM uint32_t | ESPICR

## 结构体成员变量说明

## ◆ BAUDR

__IOM uint32_t BAUDR

Baud Rate Select, Address offset: 0x014

## ◆ CR0

__IOM uint32_t CR0

Control Register 0, Address offset: 0x000

## ◆ CR1

__IOM uint32_t CR1

Control Register 1, Address offset: 0x004

## ◆ DMACR

__IOM uint32_t DMACR

DMA Control Register, Address offset: 0x04C

## ◆ DMARDLR

__IOM uint32_t DMARDLR

DMA Receive Data Level, Address offset: 0x054

## ◆ DMATDLR

__IOM uint32_t DMATDLR

DMA Transmit Data Level, Address offset: 0x050

## ◆ DR

__IOM uint32_t DR

Data Register, Address offset: 0x060

## ◆ ESPICR

__IOM uint32_t ESPICR

Enhanced SPI Control Register, Address offset: 0x0F4

## ◆ ICR

__IM uint32_t ICR

Interrupt Clear Register, Address offset: 0x048

## ◆ IER

__IOM uint32_t IER

Interrupt Enable Register, Address offset: 0x02C

## ◆ ISR

__IM uint32_t ISR

Interrupt Status Register, Address offset: 0x030

## ◆ MSTICR

__IM uint32_t MSTICR

Multi-Master Interrupt Clear Register, Address offset: 0x044

## ◆ MWCR

__IOM uint32_t MWCR

Microwire Control Register, Address offset: 0x00C

## ◆ RESERVED0

uint32_t RESERVED0[2]

Reserved, 0x058 - 0x05C

## ◆ RESERVED1

uint32_t RESERVED1[35]

Reserved, 0x064 - 0x0EC

## ◆ RISR

__IM uint32_t RISR

Raw Interrupt Status Register, Address offset: 0x034

## ◆ RX_SAMPLE_DLY

__IOM uint32_t RX_SAMPLE_DLY

RX Sample Delay Register, Address offset: 0x0F0

## ◆ RXFLR

__IM uint32_t RXFLR

Receive FIFO Level Register, Address offset: 0x024

## ◆ RXFTLR

__IOM uint32_t RXFTLR

Receive FIFO Threshold Level, Address offset: 0x01C

## ◆ RXOICR

__IM uint32_t RXOICR

Receive FIFO Overflow Interrupt Clear Register, Address offset: 0x03C

## ◆ RXUICR

__IM uint32_t RXUICR

Receive FIFO Underflow Interrupt Clear Register, Address offset: 0x040

## ◆ SER

__IOM uint32_t SER

Slave Enable Register, Address offset: 0x010

## ◆ SPIENR

__IOM uint32_t SPIENR

SPI Enable Register, Address offset: 0x008

## ◆ SR

__IM uint32_t SR

Status Register, Address offset: 0x028

## ◆ TXFLR

__IM uint32_t TXFLR

Transmit FIFO Level Register, Address offset: 0x020

## ◆ TXFTLR

__IOM uint32_t TXFTLR

Transmit FIFO Threshold Level, Address offset: 0x018

## ◆ TXOICR

__IM uint32_t TXOICR

Transmit FIFO Overflow Interrupt Clear Register, Address offset: 0x038

该结构体的文档由以下文件生成:

- wb32f10x.h