WB32F10x Standard Peripherals Firmware Library

Data Structures | Macros | Functions
wb32f10x_tim.h File Reference

This file contains all the functions prototypes for the TIM firmware library. More...

`#include "wb32f10x.h"`

Go to the source code of this file.

## Data Structures
struct | TIM_TimeBaseInitTypeDef
| TIM Time Base Init structure definition. More...
struct | TIM_OCInitTypeDef
| TIM Output Compare Init structure definition. More...
struct | TIM_ICInitTypeDef
| TIM Input Capture Init structure definition. More...
struct | TIM_BDTRInitTypeDef
| BDTR structure definition. More...

## Macros
#define | IS_TIM_ALL_PERIPH(PERIPH)
#define | IS_TIM_LIST1_PERIPH(PERIPH) ((PERIPH) == TIM1)
#define | TIM_OCMode_Timing ((uint16_t)0x0000)
#define | TIM_OCMode_Active ((uint16_t)0x0010)
#define | TIM_OCMode_Inactive ((uint16_t)0x0020)
#define | TIM_OCMode_Toggle ((uint16_t)0x0030)
#define | TIM_OCMode_PWM1 ((uint16_t)0x0060)
#define | TIM_OCMode_PWM2 ((uint16_t)0x0070)
#define | IS_TIM_OC_MODE(MODE)
#define | IS_TIM_OCM(MODE)
#define | TIM_OPMode_Single ((uint16_t)0x0008)
#define | TIM_OPMode_Repetitive ((uint16_t)0x0000)
#define | IS_TIM_OPM_MODE(MODE)
#define | TIM_Channel_1 ((uint16_t)0x0000)
#define | TIM_Channel_2 ((uint16_t)0x0004)
#define | TIM_Channel_3 ((uint16_t)0x0008)
#define | TIM_Channel_4 ((uint16_t)0x000C)
#define | IS_TIM_CHANNEL(CHANNEL)
#define | IS_TIM_PWMI_CHANNEL(CHANNEL)
#define | IS_TIM_COMPLEMENTARY_CHANNEL(CHANNEL)
#define | TIM_CKD_DIV1 ((uint16_t)0x0000)
#define | TIM_CKD_DIV2 ((uint16_t)0x0100)
#define | TIM_CKD_DIV4 ((uint16_t)0x0200)
#define | IS_TIM_CKD_DIV(DIV)
#define | TIM_CounterMode_Up ((uint16_t)0x0000)
#define | TIM_CounterMode_Down ((uint16_t)0x0010)
#define | TIM_CounterMode_CenterAligned1 ((uint16_t)0x0020)
#define | TIM_CounterMode_CenterAligned2 ((uint16_t)0x0040)
#define | TIM_CounterMode_CenterAligned3 ((uint16_t)0x0060)
#define | IS_TIM_COUNTER_MODE(MODE)
#define | TIM_OCPolarity_High ((uint16_t)0x0000)
#define | TIM_OCPolarity_Low ((uint16_t)0x0002)
#define | IS_TIM_OC_POLARITY(POLARITY)
#define | TIM_OCNPolarity_High ((uint16_t)0x0000)
#define | TIM_OCNPolarity_Low ((uint16_t)0x0008)
#define | IS_TIM_OCN_POLARITY(POLARITY)
#define | TIM_OutputState_Disable ((uint16_t)0x0000)
#define | TIM_OutputState_Enable ((uint16_t)0x0001)
#define | IS_TIM_OUTPUT_STATE(STATE)
#define | TIM_OutputNState_Disable ((uint16_t)0x0000)
#define | TIM_OutputNState_Enable ((uint16_t)0x0004)
#define | IS_TIM_OUTPUTN_STATE(STATE)
#define | TIM_CCx_Enable ((uint16_t)0x0001)
#define | TIM_CCx_Disable ((uint16_t)0x0000)
#define | IS_TIM_CCX(CCX)
#define | TIM_CCxN_Enable ((uint16_t)0x0004)
#define | TIM_CCxN_Disable ((uint16_t)0x0000)
#define | IS_TIM_CCXN(CCXN)
#define | TIM_Break_Enable ((uint16_t)0x1000)
#define | TIM_Break_Disable ((uint16_t)0x0000)
#define | IS_TIM_BREAK_STATE(STATE)
#define | TIM_BreakPolarity_Low ((uint16_t)0x0000)
#define | TIM_BreakPolarity_High ((uint16_t)0x2000)
#define | IS_TIM_BREAK_POLARITY(POLARITY)
#define | TIM_AutomaticOutput_Enable ((uint16_t)0x4000)
#define | TIM_AutomaticOutput_Disable ((uint16_t)0x0000)
#define | IS_TIM_AUTOMATIC_OUTPUT_STATE(STATE)
#define | TIM_LOCKLevel_OFF ((uint16_t)0x0000)
#define | TIM_LOCKLevel_1 ((uint16_t)0x0100)
#define | TIM_LOCKLevel_2 ((uint16_t)0x0200)
#define | TIM_LOCKLevel_3 ((uint16_t)0x0300)
#define | IS_TIM_LOCK_LEVEL(LEVEL)
#define | TIM_OSSIState_Enable ((uint16_t)0x0400)
#define | TIM_OSSIState_Disable ((uint16_t)0x0000)
#define | IS_TIM_OSSI_STATE(STATE)
#define | TIM_OSSRState_Enable ((uint16_t)0x0800)
#define | TIM_OSSRState_Disable ((uint16_t)0x0000)
#define | IS_TIM_OSSR_STATE(STATE)
#define | TIM_OCIdleState_Set ((uint16_t)0x0100)
#define | TIM_OCIdleState_Reset ((uint16_t)0x0000)
#define | IS_TIM_OCIDLE_STATE(STATE)
#define | TIM_OCNIdleState_Set ((uint16_t)0x0200)
#define | TIM_OCNIdleState_Reset ((uint16_t)0x0000)
#define | IS_TIM_OCNIDLE_STATE(STATE)
#define | TIM_ICPolarity_Rising ((uint16_t)0x0000)
#define | TIM_ICPolarity_Falling ((uint16_t)0x0002)
#define | TIM_ICPolarity_BothEdge ((uint16_t)0x000A)
#define | IS_TIM_IC_POLARITY(POLARITY)
#define | TIM_ICSelection_DirectTI ((uint16_t)0x0001)
#define | TIM_ICSelection_IndirectTI ((uint16_t)0x0002)
#define | TIM_ICSelection_TRC ((uint16_t)0x0003)
#define | IS_TIM_IC_SELECTION(SELECTION)
#define | TIM_ICPSC_DIV1 ((uint16_t)0x0000)
#define | TIM_ICPSC_DIV2 ((uint16_t)0x0004)
#define | TIM_ICPSC_DIV4 ((uint16_t)0x0008)
#define | TIM_ICPSC_DIV8 ((uint16_t)0x000C)
#define | IS_TIM_IC_PRESCALER(PRESCALER)
#define | TIM_IT_Update ((uint16_t)0x0001)
#define | TIM_IT_CC1 ((uint16_t)0x0002)
#define | TIM_IT_CC2 ((uint16_t)0x0004)
#define | TIM_IT_CC3 ((uint16_t)0x0008)
#define | TIM_IT_CC4 ((uint16_t)0x0010)
#define | TIM_IT_COM ((uint16_t)0x0020)
#define | TIM_IT_Trigger ((uint16_t)0x0040)
#define | TIM_IT_Break ((uint16_t)0x0080)
#define | IS_TIM_IT(IT) ((((IT) & (uint16_t)0xFF00) == 0x0000) && ((IT) != 0x0000))
#define | IS_TIM_GET_IT(IT)
#define | TIM_DMA_Update ((uint16_t)0x0100)
#define | TIM_DMA_CC1 ((uint16_t)0x0200)
#define | TIM_DMA_CC2 ((uint16_t)0x0400)
#define | TIM_DMA_CC3 ((uint16_t)0x0800)
#define | TIM_DMA_CC4 ((uint16_t)0x1000)
#define | TIM_DMA_COM ((uint16_t)0x2000)
#define | TIM_DMA_Trigger ((uint16_t)0x4000)
#define | IS_TIM_DMA_SOURCE(SOURCE) ((((SOURCE) & (uint16_t)0x80FF) == 0x0000) && ((SOURCE) != 0x0000))
#define | TIM_ExtTRGPSC_OFF ((uint16_t)0x0000)
#define | TIM_ExtTRGPSC_DIV2 ((uint16_t)0x1000)
#define | TIM_ExtTRGPSC_DIV4 ((uint16_t)0x2000)
#define | TIM_ExtTRGPSC_DIV8 ((uint16_t)0x3000)
#define | IS_TIM_EXT_PRESCALER(PRESCALER)
#define | TIM_TS_ITR0 ((uint16_t)0x0000)
#define | TIM_TS_ITR1 ((uint16_t)0x0010)
#define | TIM_TS_ITR2 ((uint16_t)0x0020)
#define | TIM_TS_ITR3 ((uint16_t)0x0030)
#define | TIM_TS_TI1F_ED ((uint16_t)0x0040)
#define | TIM_TS_TI1FP1 ((uint16_t)0x0050)
#define | TIM_TS_TI2FP2 ((uint16_t)0x0060)
#define | TIM_TS_ETRF ((uint16_t)0x0070)
#define | IS_TIM_TRIGGER_SELECTION(SELECTION)
#define | IS_TIM_INTERNAL_TRIGGER_SELECTION(SELECTION)
#define | TIM_TIxExternalCLK1Source_TI1 ((uint16_t)0x0050)
#define | TIM_TIxExternalCLK1Source_TI2 ((uint16_t)0x0060)
#define | TIM_TIxExternalCLK1Source_TI1ED ((uint16_t)0x0040)
#define | IS_TIM_TIXCLK_SOURCE(SOURCE)
#define | TIM_ExtTRGPolarity_Inverted ((uint16_t)0x8000)
#define | TIM_ExtTRGPolarity_NonInverted ((uint16_t)0x0000)
#define | IS_TIM_EXT_POLARITY(POLARITY)
#define | TIM_PSCReloadMode_Update ((uint16_t)0x0000)
#define | TIM_PSCReloadMode_Immediate ((uint16_t)0x0001)
#define | IS_TIM_PRESCALER_RELOAD(RELOAD)
#define | TIM_ForcedAction_Active ((uint16_t)0x0050)
#define | TIM_ForcedAction_InActive ((uint16_t)0x0040)
#define | IS_TIM_FORCED_ACTION(ACTION)
#define | TIM_EncoderMode_TI1 ((uint16_t)0x0001)
#define | TIM_EncoderMode_TI2 ((uint16_t)0x0002)
#define | TIM_EncoderMode_TI12 ((uint16_t)0x0003)
#define | IS_TIM_ENCODER_MODE(MODE)
#define | TIM_EventSource_Update ((uint16_t)0x0001)
#define | TIM_EventSource_CC1 ((uint16_t)0x0002)
#define | TIM_EventSource_CC2 ((uint16_t)0x0004)
#define | TIM_EventSource_CC3 ((uint16_t)0x0008)
#define | TIM_EventSource_CC4 ((uint16_t)0x0010)
#define | TIM_EventSource_COM ((uint16_t)0x0020)
#define | TIM_EventSource_Trigger ((uint16_t)0x0040)
#define | TIM_EventSource_Break ((uint16_t)0x0080)
#define | IS_TIM_EVENT_SOURCE(SOURCE) ((((SOURCE) & (uint16_t)0xFF00) == 0x0000) && ((SOURCE) != 0x0000))
#define | TIM_UpdateSource_Global ((uint16_t)0x0000)
#define | TIM_UpdateSource_Regular ((uint16_t)0x0001)
#define | IS_TIM_UPDATE_SOURCE(SOURCE)
#define | TIM_OCPreload_Enable ((uint16_t)0x0008)
#define | TIM_OCPreload_Disable ((uint16_t)0x0000)
#define | IS_TIM_OCPRELOAD_STATE(STATE)
#define | TIM_OCFast_Enable ((uint16_t)0x0004)
#define | TIM_OCFast_Disable ((uint16_t)0x0000)
#define | IS_TIM_OCFAST_STATE(STATE)
#define | TIM_OCClear_Enable ((uint16_t)0x0080)
#define | TIM_OCClear_Disable ((uint16_t)0x0000)
#define | IS_TIM_OCCLEAR_STATE(STATE)
#define | TIM_TRGOSource_Reset ((uint16_t)0x0000)
#define | TIM_TRGOSource_Enable ((uint16_t)0x0010)
#define | TIM_TRGOSource_Update ((uint16_t)0x0020)
#define | TIM_TRGOSource_OC1 ((uint16_t)0x0030)
#define | TIM_TRGOSource_OC1Ref ((uint16_t)0x0040)
#define | TIM_TRGOSource_OC2Ref ((uint16_t)0x0050)
#define | TIM_TRGOSource_OC3Ref ((uint16_t)0x0060)
#define | TIM_TRGOSource_OC4Ref ((uint16_t)0x0070)
#define | IS_TIM_TRGO_SOURCE(SOURCE)
#define | TIM_SlaveMode_Reset ((uint16_t)0x0004)
#define | TIM_SlaveMode_Gated ((uint16_t)0x0005)
#define | TIM_SlaveMode_Trigger ((uint16_t)0x0006)
#define | TIM_SlaveMode_External1 ((uint16_t)0x0007)
#define | IS_TIM_SLAVE_MODE(MODE)
#define | TIM_MasterSlaveMode_Enable ((uint16_t)0x0080)
#define | TIM_MasterSlaveMode_Disable ((uint16_t)0x0000)
#define | IS_TIM_MSM_STATE(STATE)
#define | TIM_FLAG_Update ((uint16_t)0x0001)
#define | TIM_FLAG_CC1 ((uint16_t)0x0002)
#define | TIM_FLAG_CC2 ((uint16_t)0x0004)
#define | TIM_FLAG_CC3 ((uint16_t)0x0008)
#define | TIM_FLAG_CC4 ((uint16_t)0x0010)
#define | TIM_FLAG_COM ((uint16_t)0x0020)
#define | TIM_FLAG_Trigger ((uint16_t)0x0040)
#define | TIM_FLAG_Break ((uint16_t)0x0080)
#define | TIM_FLAG_CC1OF ((uint16_t)0x0200)
#define | TIM_FLAG_CC2OF ((uint16_t)0x0400)
#define | TIM_FLAG_CC3OF ((uint16_t)0x0800)
#define | TIM_FLAG_CC4OF ((uint16_t)0x1000)
#define | IS_TIM_GET_FLAG(FLAG)
#define | IS_TIM_CLEAR_FLAG(TIM_FLAG) ((((TIM_FLAG) & (uint16_t)0xE100) == 0x0000) && ((TIM_FLAG) != 0x0000))
#define | IS_TIM_IC_FILTER(ICFILTER) ((ICFILTER) <= 0xF)
#define | IS_TIM_EXT_FILTER(EXTFILTER) ((EXTFILTER) <= 0xF)

## Functions
void | TIM_DeInit (TIM_TypeDef *TIMx)
| Deinitializes the TIMx peripheral registers to their default reset values. More...
void | TIM_TimeBaseInit (TIM_TypeDef *TIMx, TIM_TimeBaseInitTypeDef *TIM_TimeBaseInitStruct)
| Initializes the TIMx Time Base Unit peripheral according to the specified parameters in the TIM_TimeBaseInitStruct. More...
void | TIM_OC1Init (TIM_TypeDef *TIMx, TIM_OCInitTypeDef *TIM_OCInitStruct)
| Initializes the TIMx Channel1 according to the specified parameters in the TIM_OCInitStruct. More...
void | TIM_OC2Init (TIM_TypeDef *TIMx, TIM_OCInitTypeDef *TIM_OCInitStruct)
| Initializes the TIMx Channel2 according to the specified parameters in the TIM_OCInitStruct. More...
void | TIM_OC3Init (TIM_TypeDef *TIMx, TIM_OCInitTypeDef *TIM_OCInitStruct)
| Initializes the TIMx Channel3 according to the specified parameters in the TIM_OCInitStruct. More...
void | TIM_OC4Init (TIM_TypeDef *TIMx, TIM_OCInitTypeDef *TIM_OCInitStruct)
| Initializes the TIMx Channel4 according to the specified parameters in the TIM_OCInitStruct. More...
void | TIM_ICInit (TIM_TypeDef *TIMx, TIM_ICInitTypeDef *TIM_ICInitStruct)
| Initializes the TIM peripheral according to the specified parameters in the TIM_ICInitStruct. More...
void | TIM_PWMIConfig (TIM_TypeDef *TIMx, TIM_ICInitTypeDef *TIM_ICInitStruct)
| Configures the TIM peripheral according to the specified parameters in the TIM_ICInitStruct to measure an external PWM signal. More...
void | TIM_BDTRConfig (TIM_TypeDef *TIMx, TIM_BDTRInitTypeDef *TIM_BDTRInitStruct)
| Configures the: Break feature, dead time, Lock level, the OSSI, the OSSR State and the AOE(automatic output enable). More...
void | TIM_TimeBaseStructInit (TIM_TimeBaseInitTypeDef *TIM_TimeBaseInitStruct)
| Fills each TIM_TimeBaseInitStruct member with its default value. More...
void | TIM_OCStructInit (TIM_OCInitTypeDef *TIM_OCInitStruct)
| Fills each TIM_OCInitStruct member with its default value. More...
void | TIM_ICStructInit (TIM_ICInitTypeDef *TIM_ICInitStruct)
| Fills each TIM_ICInitStruct member with its default value. More...
void | TIM_BDTRStructInit (TIM_BDTRInitTypeDef *TIM_BDTRInitStruct)
| Fills each TIM_BDTRInitStruct member with its default value. More...
void | TIM_Cmd (TIM_TypeDef *TIMx, FunctionalState NewState)
| Enables or disables the specified TIM peripheral. More...
void | TIM_CtrlPWMOutputs (TIM_TypeDef *TIMx, FunctionalState NewState)
| Enables or disables the TIM peripheral Main Outputs. More...
void | TIM_ITConfig (TIM_TypeDef *TIMx, uint16_t TIM_IT, FunctionalState NewState)
| Enables or disables the specified TIM interrupts. More...
void | TIM_GenerateEvent (TIM_TypeDef *TIMx, uint16_t TIM_EventSource)
| Configures the TIMx event to be generate by software. More...
void | TIM_DMACmd (TIM_TypeDef *TIMx, uint16_t TIM_DMASource, FunctionalState NewState)
| Enables or disables the TIMx's DMA Requests. More...
void | TIM_InternalClockConfig (TIM_TypeDef *TIMx)
| Configures the TIMx internal Clock. More...
void | TIM_ITRxExternalClockConfig (TIM_TypeDef *TIMx, uint16_t TIM_InputTriggerSource)
| Configures the TIMx Internal Trigger as External Clock. More...
void | TIM_TIxExternalClockConfig (TIM_TypeDef *TIMx, uint16_t TIM_TIxExternalCLKSource, uint16_t TIM_ICPolarity, uint16_t ICFilter)
| Configures the TIMx Trigger as External Clock. More...
void | TIM_ETRClockMode1Config (TIM_TypeDef *TIMx, uint16_t TIM_ExtTRGPrescaler, uint16_t TIM_ExtTRGPolarity, uint16_t ExtTRGFilter)
| Configures the External clock Mode1. More...
void | TIM_ETRClockMode2Config (TIM_TypeDef *TIMx, uint16_t TIM_ExtTRGPrescaler, uint16_t TIM_ExtTRGPolarity, uint16_t ExtTRGFilter)
| Configures the External clock Mode2. More...
void | TIM_ETRConfig (TIM_TypeDef *TIMx, uint16_t TIM_ExtTRGPrescaler, uint16_t TIM_ExtTRGPolarity, uint16_t ExtTRGFilter)
| Configures the TIMx External Trigger (ETR). More...
void | TIM_PrescalerConfig (TIM_TypeDef *TIMx, uint16_t Prescaler, uint16_t TIM_PSCReloadMode)
| Configures the TIMx Prescaler. More...
void | TIM_CounterModeConfig (TIM_TypeDef *TIMx, uint16_t TIM_CounterMode)
| Specifies the TIMx Counter Mode to be used. More...
void | TIM_SelectInputTrigger (TIM_TypeDef *TIMx, uint16_t TIM_InputTriggerSource)
| Selects the Input Trigger source. More...
void | TIM_EncoderInterfaceConfig (TIM_TypeDef *TIMx, uint16_t TIM_EncoderMode, uint16_t TIM_IC1Polarity, uint16_t TIM_IC2Polarity)
| Configures the TIMx Encoder Interface. More...
void | TIM_ForcedOC1Config (TIM_TypeDef *TIMx, uint16_t TIM_ForcedAction)
| Forces the TIMx output 1 waveform to active or inactive level. More...
void | TIM_ForcedOC2Config (TIM_TypeDef *TIMx, uint16_t TIM_ForcedAction)
| Forces the TIMx output 2 waveform to active or inactive level. More...
void | TIM_ForcedOC3Config (TIM_TypeDef *TIMx, uint16_t TIM_ForcedAction)
| Forces the TIMx output 3 waveform to active or inactive level. More...
void | TIM_ForcedOC4Config (TIM_TypeDef *TIMx, uint16_t TIM_ForcedAction)
| Forces the TIMx output 4 waveform to active or inactive level. More...
void | TIM_ARRPreloadConfig (TIM_TypeDef *TIMx, FunctionalState NewState)
| Enables or disables TIMx peripheral Preload register on ARR. More...
void | TIM_SelectCOM (TIM_TypeDef *TIMx, FunctionalState NewState)
| Selects the TIM peripheral Commutation event. More...
void | TIM_SelectCCDMA (TIM_TypeDef *TIMx, FunctionalState NewState)
| Selects the TIMx peripheral Capture Compare DMA source. More...
void | TIM_CCPreloadControl (TIM_TypeDef *TIMx, FunctionalState NewState)
| Sets or Resets the TIM peripheral Capture Compare Preload Control bit. More...
void | TIM_OC1PreloadConfig (TIM_TypeDef *TIMx, uint16_t TIM_OCPreload)
| Enables or disables the TIMx peripheral Preload register on CCR1. More...
void | TIM_OC2PreloadConfig (TIM_TypeDef *TIMx, uint16_t TIM_OCPreload)
| Enables or disables the TIMx peripheral Preload register on CCR2. More...
void | TIM_OC3PreloadConfig (TIM_TypeDef *TIMx, uint16_t TIM_OCPreload)
| Enables or disables the TIMx peripheral Preload register on CCR3. More...
void | TIM_OC4PreloadConfig (TIM_TypeDef *TIMx, uint16_t TIM_OCPreload)
| Enables or disables the TIMx peripheral Preload register on CCR4. More...
void | TIM_OC1FastConfig (TIM_TypeDef *TIMx, uint16_t TIM_OCFast)
| Configures the TIMx Output Compare 1 Fast feature. More...
void | TIM_OC2FastConfig (TIM_TypeDef *TIMx, uint16_t TIM_OCFast)
| Configures the TIMx Output Compare 2 Fast feature. More...
void | TIM_OC3FastConfig (TIM_TypeDef *TIMx, uint16_t TIM_OCFast)
| Configures the TIMx Output Compare 3 Fast feature. More...
void | TIM_OC4FastConfig (TIM_TypeDef *TIMx, uint16_t TIM_OCFast)
| Configures the TIMx Output Compare 4 Fast feature. More...
void | TIM_ClearOC1Ref (TIM_TypeDef *TIMx, uint16_t TIM_OCClear)
| Clears or safeguards the OCREF1 signal on an external event. More...
void | TIM_ClearOC2Ref (TIM_TypeDef *TIMx, uint16_t TIM_OCClear)
| Clears or safeguards the OCREF2 signal on an external event. More...
void | TIM_ClearOC3Ref (TIM_TypeDef *TIMx, uint16_t TIM_OCClear)
| Clears or safeguards the OCREF3 signal on an external event. More...
void | TIM_ClearOC4Ref (TIM_TypeDef *TIMx, uint16_t TIM_OCClear)
| Clears or safeguards the OCREF4 signal on an external event. More...
void | TIM_OC1PolarityConfig (TIM_TypeDef *TIMx, uint16_t TIM_OCPolarity)
| Configures the TIMx channel 1 polarity. More...
void | TIM_OC1NPolarityConfig (TIM_TypeDef *TIMx, uint16_t TIM_OCNPolarity)
| Configures the TIMx Channel 1N polarity. More...
void | TIM_OC2PolarityConfig (TIM_TypeDef *TIMx, uint16_t TIM_OCPolarity)
| Configures the TIMx channel 2 polarity. More...
void | TIM_OC2NPolarityConfig (TIM_TypeDef *TIMx, uint16_t TIM_OCNPolarity)
| Configures the TIMx Channel 2N polarity. More...
void | TIM_OC3PolarityConfig (TIM_TypeDef *TIMx, uint16_t TIM_OCPolarity)
| Configures the TIMx channel 3 polarity. More...
void | TIM_OC3NPolarityConfig (TIM_TypeDef *TIMx, uint16_t TIM_OCNPolarity)
| Configures the TIMx Channel 3N polarity. More...
void | TIM_OC4PolarityConfig (TIM_TypeDef *TIMx, uint16_t TIM_OCPolarity)
| Configures the TIMx channel 4 polarity. More...
void | TIM_CCxCmd (TIM_TypeDef *TIMx, uint16_t TIM_Channel, uint16_t TIM_CCx)
| Enables or disables the TIM Capture Compare Channel x. More...
void | TIM_CCxNCmd (TIM_TypeDef *TIMx, uint16_t TIM_Channel, uint16_t TIM_CCxN)
| Enables or disables the TIM Capture Compare Channel xN. More...
void | TIM_SelectOCxM (TIM_TypeDef *TIMx, uint16_t TIM_Channel, uint16_t TIM_OCMode)
| Selects the TIM Output Compare Mode. More...
void | TIM_UpdateDisableConfig (TIM_TypeDef *TIMx, FunctionalState NewState)
| Enables or Disables the TIMx Update event. More...
void | TIM_UpdateRequestConfig (TIM_TypeDef *TIMx, uint16_t TIM_UpdateSource)
| Configures the TIMx Update Request Interrupt source. More...
void | TIM_SelectHallSensor (TIM_TypeDef *TIMx, FunctionalState NewState)
| Enables or disables the TIMx's Hall sensor interface. More...
void | TIM_SelectOnePulseMode (TIM_TypeDef *TIMx, uint16_t TIM_OPMode)
| Selects the TIMx's One Pulse Mode. More...
void | TIM_SelectOutputTrigger (TIM_TypeDef *TIMx, uint16_t TIM_TRGOSource)
| Selects the TIMx Trigger Output Mode. More...
void | TIM_SelectSlaveMode (TIM_TypeDef *TIMx, uint16_t TIM_SlaveMode)
| Selects the TIMx Slave Mode. More...
void | TIM_SelectMasterSlaveMode (TIM_TypeDef *TIMx, uint16_t TIM_MasterSlaveMode)
| Sets or Resets the TIMx Master/Slave Mode. More...
void | TIM_SetCounter (TIM_TypeDef *TIMx, uint32_t Counter)
| Sets the TIMx Counter Register value. More...
void | TIM_SetAutoreload (TIM_TypeDef *TIMx, uint32_t Autoreload)
| Sets the TIMx Autoreload Register value. More...
void | TIM_SetCompare1 (TIM_TypeDef *TIMx, uint32_t Compare1)
| Sets the TIMx Capture Compare1 Register value. More...
void | TIM_SetCompare2 (TIM_TypeDef *TIMx, uint32_t Compare2)
| Sets the TIMx Capture Compare2 Register value. More...
void | TIM_SetCompare3 (TIM_TypeDef *TIMx, uint32_t Compare3)
| Sets the TIMx Capture Compare3 Register value. More...
void | TIM_SetCompare4 (TIM_TypeDef *TIMx, uint32_t Compare4)
| Sets the TIMx Capture Compare4 Register value. More...
void | TIM_SetIC1Prescaler (TIM_TypeDef *TIMx, uint16_t TIM_ICPSC)
| Sets the TIMx Input Capture 1 prescaler. More...
void | TIM_SetIC2Prescaler (TIM_TypeDef *TIMx, uint16_t TIM_ICPSC)
| Sets the TIMx Input Capture 2 prescaler. More...
void | TIM_SetIC3Prescaler (TIM_TypeDef *TIMx, uint16_t TIM_ICPSC)
| Sets the TIMx Input Capture 3 prescaler. More...
void | TIM_SetIC4Prescaler (TIM_TypeDef *TIMx, uint16_t TIM_ICPSC)
| Sets the TIMx Input Capture 4 prescaler. More...
void | TIM_SetClockDivision (TIM_TypeDef *TIMx, uint16_t TIM_CKD)
| Sets the TIMx Clock Division value. More...
uint32_t | TIM_GetCapture1 (TIM_TypeDef *TIMx)
| Gets the TIMx Input Capture 1 value. More...
uint32_t | TIM_GetCapture2 (TIM_TypeDef *TIMx)
| Gets the TIMx Input Capture 2 value. More...
uint32_t | TIM_GetCapture3 (TIM_TypeDef *TIMx)
| Gets the TIMx Input Capture 3 value. More...
uint32_t | TIM_GetCapture4 (TIM_TypeDef *TIMx)
| Gets the TIMx Input Capture 4 value. More...
uint32_t | TIM_GetCounter (TIM_TypeDef *TIMx)
| Gets the TIMx Counter value. More...
uint16_t | TIM_GetPrescaler (TIM_TypeDef *TIMx)
| Gets the TIMx Prescaler value. More...
FlagStatus | TIM_GetFlagStatus (TIM_TypeDef *TIMx, uint16_t TIM_FLAG)
| Checks whether the specified TIM flag is set or not. More...
void | TIM_ClearFlag (TIM_TypeDef *TIMx, uint16_t TIM_FLAG)
| Clears the TIMx's pending flags. More...
ITStatus | TIM_GetITStatus (TIM_TypeDef *TIMx, uint16_t TIM_IT)
| Checks whether the TIM interrupt has occurred or not. More...
void | TIM_ClearITPendingBit (TIM_TypeDef *TIMx, uint16_t TIM_IT)
| Clears the TIMx's interrupt pending bits. More...

## Detailed Description

This file contains all the functions prototypes for the TIM firmware library.

Author
  Westberry Application Team

Version
  V0.1.10

Date
  05-January-2023