WB32F10x Standard Peripherals Firmware Library

Data Fields
NVIC_InitTypeDef Struct Reference
WB32F10x_StdPeriph_Driver » MISC » MISC_Exported_Types

NVIC Init Structure definition. More...

`#include <misc.h>`

## Data Fields
uint8_t | NVIC_IRQChannel
uint8_t | NVIC_IRQChannelPreemptionPriority
uint8_t | NVIC_IRQChannelSubPriority
FunctionalState | NVIC_IRQChannelCmd

## Detailed Description

NVIC Init Structure definition.

## Field Documentation

## ◆ NVIC_IRQChannel

uint8_t NVIC_IRQChannel

Specifies the IRQ channel to be enabled or disabled. This parameter can be a value of IRQn_Type (For the complete WB32 Devices IRQ Channels list, please refer to wb32f10x.h file)

## ◆ NVIC_IRQChannelCmd

FunctionalState NVIC_IRQChannelCmd

Specifies whether the IRQ channel defined in NVIC_IRQChannel will be enabled or disabled. This parameter can be set either to ENABLE or DISABLE

## ◆ NVIC_IRQChannelPreemptionPriority

uint8_t NVIC_IRQChannelPreemptionPriority

Specifies the pre-emption priority for the IRQ channel specified in NVIC_IRQChannel. This parameter can be a value between 0 and 15 as described in the table NVIC_Priority_Table

## ◆ NVIC_IRQChannelSubPriority

uint8_t NVIC_IRQChannelSubPriority

Specifies the subpriority level for the IRQ channel specified in NVIC_IRQChannel. This parameter can be a value between 0 and 15 as described in the table NVIC_Priority_Table

The documentation for this struct was generated from the following file:

- misc.h