WB32F10x Standard Peripherals Firmware Library

Data Fields
PWR_TypeDef Struct Reference
CMSIS » Wb32f10x

## Data Fields
__IOM uint32_t | CR0
__OM uint32_t | CR1
__IOM uint32_t | CR2
uint32_t | RESERVED0
__IM uint32_t | SR0
__IM uint32_t | SR1
__IOM uint32_t | GPREG0
__IOM uint32_t | GPREG1
__IOM uint32_t | CFGR
uint32_t | RESERVED1
__OM uint32_t | ANAKEY1
__OM uint32_t | ANAKEY2

## Field Documentation

## ◆ ANAKEY1

__OM uint32_t ANAKEY1

ANCTL write enable key register 0, Address offset: 0x028

## ◆ ANAKEY2

__OM uint32_t ANAKEY2

ANCTL write enable key register 1, Address offset: 0x02C

## ◆ CFGR

__IOM uint32_t CFGR

PWR configuration register, Address offset: 0x020

## ◆ CR0

__IOM uint32_t CR0

Control register 0, Address offset: 0x000

## ◆ CR1

__OM uint32_t CR1

Control register 1, Address offset: 0x004

## ◆ CR2

__IOM uint32_t CR2

Control register 2, Address offset: 0x008

## ◆ GPREG0

__IOM uint32_t GPREG0

General purpose register 0, Address offset: 0x018

## ◆ GPREG1

__IOM uint32_t GPREG1

General purpose register 1, Address offset: 0x01C

## ◆ RESERVED0

uint32_t RESERVED0

Reserved, 0x00C

## ◆ RESERVED1

uint32_t RESERVED1

Reserved, 0x024

## ◆ SR0

__IM uint32_t SR0

Status register 0, Address offset: 0x010

## ◆ SR1

__IM uint32_t SR1

Status register 1, Address offset: 0x014

The documentation for this struct was generated from the following file:

- wb32f10x.h