WB32F10x Standard Peripherals Firmware Library

成员变量
NVIC_InitTypeDef结构体 参考
WB32F10x_StdPeriph_Driver » MISC » MISC_Exported_Types

NVIC Init Structure definition 更多...

`#include <misc.h>`

## 成员变量
uint8_t | NVIC_IRQChannel
uint8_t | NVIC_IRQChannelPreemptionPriority
uint8_t | NVIC_IRQChannelSubPriority
FunctionalState | NVIC_IRQChannelCmd

## 详细描述

NVIC Init Structure definition

## 结构体成员变量说明

## ◆ NVIC_IRQChannel

uint8_t NVIC_IRQChannel

Specifies the IRQ channel to be enabled or disabled. This parameter can be a value of IRQn_Type (For the complete WB32 Devices IRQ Channels list, please refer to wb32f10x.h file)

## ◆ NVIC_IRQChannelCmd

FunctionalState NVIC_IRQChannelCmd

Specifies whether the IRQ channel defined in NVIC_IRQChannel will be enabled or disabled. This parameter can be set either to ENABLE or DISABLE

## ◆ NVIC_IRQChannelPreemptionPriority

uint8_t NVIC_IRQChannelPreemptionPriority

Specifies the pre-emption priority for the IRQ channel specified in NVIC_IRQChannel. This parameter can be a value between 0 and 15 as described in the table NVIC_Priority_Table

## ◆ NVIC_IRQChannelSubPriority

uint8_t NVIC_IRQChannelSubPriority

Specifies the subpriority level for the IRQ channel specified in NVIC_IRQChannel. This parameter can be a value between 0 and 15 as described in the table NVIC_Priority_Table

该结构体的文档由以下文件生成:

- misc.h