WB32F10x Standard Peripherals Firmware Library

Data Fields
ISO_TypeDef Struct Reference
CMSIS » Wb32f10x

## Data Fields
__OM uint32_t | TXBUF
__IM uint32_t | RXBUF
__IOM uint32_t | TXDONE
__IOM uint32_t | RXDONE
__IOM uint32_t | STARTDET
__IM uint32_t | CLRTXDONE
__IM uint32_t | CLRRXDONE
__IM uint32_t | CLRSTART
__IOM uint32_t | TRANSR
__IOM uint32_t | FIFOSR
__IOM uint32_t | IER
__IOM uint32_t | MODE
__IOM uint32_t | ETU
__IM uint32_t | RISR
__IM uint32_t | ISR

## Field Documentation

## ◆ CLRRXDONE

__IM uint32_t CLRRXDONE

ISO7816 register, Address offset: 0x018

## ◆ CLRSTART

__IM uint32_t CLRSTART

ISO7816 register, Address offset: 0x01C

## ◆ CLRTXDONE

__IM uint32_t CLRTXDONE

ISO7816 register, Address offset: 0x014

## ◆ ETU

__IOM uint32_t ETU

ISO7816 register, Address offset: 0x030

## ◆ FIFOSR

__IOM uint32_t FIFOSR

ISO7816 register, Address offset: 0x024

## ◆ IER

__IOM uint32_t IER

ISO7816 register, Address offset: 0x028

## ◆ ISR

__IM uint32_t ISR

ISO7816 register, Address offset: 0x038

## ◆ MODE

__IOM uint32_t MODE

ISO7816 register, Address offset: 0x02C

## ◆ RISR

__IM uint32_t RISR

ISO7816 register, Address offset: 0x034

## ◆ RXBUF

__IM uint32_t RXBUF

ISO7816 register, Address offset: 0x004

## ◆ RXDONE

__IOM uint32_t RXDONE

ISO7816 register, Address offset: 0x00C

## ◆ STARTDET

__IOM uint32_t STARTDET

ISO7816 register, Address offset: 0x010

## ◆ TRANSR

__IOM uint32_t TRANSR

ISO7816 register, Address offset: 0x020

## ◆ TXBUF

__OM uint32_t TXBUF

ISO7816 register, Address offset: 0x000

## ◆ TXDONE

__IOM uint32_t TXDONE

ISO7816 register, Address offset: 0x008

The documentation for this struct was generated from the following file:

- wb32f10x.h