WB32F10x Standard Peripherals Firmware Library

枚举 | 函数
usbd_intr.c 文件参考
`#include "wb32f10x.h"`
`#include <stdlib.h>`
`#include "usbd_core.h"`
`#include "usbd_user.h"`

## 枚举
enum | Endpoint0State_t { EP0_STATE_IDLE, EP0_STATE_TX, EP0_STATE_RX, EP0_STATE_STALL }

## 函数
void | USBD_EndPoint0 (void)
| Handle Endpoint 0 Event 更多...
void | Handle_USBD_INT (uint8_t IntrUSB, uint8_t IntrIn, uint8_t IntrOut)
| Handle USBD Interrupts. 更多...

## 详细描述

作者
  Westberry Application Team

注意

Copyright (c) 2020 - 2023 Westberry Technology (ChangZhou) Corp., Ltd All rights reserved.

THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME. AS A RESULT, WESTBERRY TECHNOLOGY SHALL NOT BE HELD LIABLE FOR ANY DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.

## 函数说明

## ◆ Handle_USBD_INT()

void Handle_USBD_INT | ( | uint8_t | IntrUSB,
|  | uint8_t | IntrIn,
|  | uint8_t | IntrOut
| ) |  |

Handle USBD Interrupts.

返回
  None

## ◆ USBD_EndPoint0()

void USBD_EndPoint0 | ( | void |  | ) |

Handle Endpoint 0 Event

返回
  None