WB32F10x Standard Peripherals Firmware Library

成员变量
I2C_TypeDef结构体 参考
CMSIS » Wb32f10x

## 成员变量
__IOM uint32_t | CON
__IOM uint32_t | TAR
__IOM uint32_t | SAR
__IOM uint32_t | HS_MADDR
__IOM uint32_t | DATA_CMD
__IOM uint32_t | SS_SCL_HCNT
__IOM uint32_t | SS_SCL_LCNT
__IOM uint32_t | FS_SCL_HCNT
__IOM uint32_t | FS_SCL_LCNT
__IOM uint32_t | HS_SCL_HCNT
__IOM uint32_t | HS_SCL_LCNT
__IM uint32_t | INTR_STAT
__IOM uint32_t | INTR_MASK
__IM uint32_t | RAW_INTR_STAT
__IOM uint32_t | RX_TL
__IOM uint32_t | TX_TL
__IM uint32_t | CLR_INTR
__IM uint32_t | CLR_RX_UNDER
__IM uint32_t | CLR_RX_OVER
__IM uint32_t | CLR_TX_OVER
__IM uint32_t | CLR_RD_REQ
__IM uint32_t | CLR_TX_ABRT
__IM uint32_t | CLR_RX_DONE
__IM uint32_t | CLR_ACTIVITY
__IM uint32_t | CLR_STOP_DET
__IM uint32_t | CLR_START_DET
__IM uint32_t | CLR_GEN_CALL
__IOM uint32_t | ENABLE
__IM uint32_t | STATUS
__IM uint32_t | TXFLR
__IM uint32_t | RXFLR
__IOM uint32_t | SDA_HOLD
__IM uint32_t | TX_ABRT_SOURCE
__IOM uint32_t | SLV_DATA_NACK_ONLY
__IOM uint32_t | DMA_CR
__IOM uint32_t | DMA_TDLR
__IOM uint32_t | DMA_RDLR
__IOM uint32_t | SDA_SETUP
__IOM uint32_t | ACK_GENERAL_CALL
__IM uint32_t | ENABLE_STATUS
__IOM uint32_t | FS_SPKLEN
__IOM uint32_t | HS_SPKLEN
__IM uint32_t | CLR_RESTART_DET
__IOM uint32_t | SCL_STUCK_AT_LOW_TIMEOUT
__IOM uint32_t | SDA_STUCK_AT_LOW_TIMEOUT
__IM uint32_t | CLR_SCL_STUCK_DET
uint32_t | RESERVED0
__IOM uint32_t | SMBUS_CLK_LOW_SEXT
__IOM uint32_t | SMBUS_CLK_LOW_MEXT
__IOM uint32_t | SMBUS_THIGH_MAX_IDLE_COUNT
__IM uint32_t | SMBUS_INTR_STAT
__IOM uint32_t | SMBUS_INTR_MASK
__IM uint32_t | SMBUS_RAW_INTR_STAT
__OM uint32_t | CLR_SMBUS_INTR
__IOM uint32_t | OPTIONAL_SAR
__IOM uint32_t | SMBUS_UDID_LSB

## 结构体成员变量说明

## ◆ ACK_GENERAL_CALL

__IOM uint32_t ACK_GENERAL_CALL

I2C ACK General Call Register, Address offset: 0x098

## ◆ CLR_ACTIVITY

__IM uint32_t CLR_ACTIVITY

Clear ACTIVITY Interrupt Register, Address offset: 0x05C

## ◆ CLR_GEN_CALL

__IM uint32_t CLR_GEN_CALL

Clear GEN_CALL Interrupt Register, Address offset: 0x068

## ◆ CLR_INTR

__IM uint32_t CLR_INTR

Clear Combined and Individual Interrupt Register, Address offset: 0x040

## ◆ CLR_RD_REQ

__IM uint32_t CLR_RD_REQ

Clear RD_REQ Interrupt Register, Address offset: 0x050

## ◆ CLR_RESTART_DET

__IM uint32_t CLR_RESTART_DET

Clear RESTART_DET Interrupt Register, Address offset: 0x0A8

## ◆ CLR_RX_DONE

__IM uint32_t CLR_RX_DONE

Clear RX_DONE Interrupt Register, Address offset: 0x058

## ◆ CLR_RX_OVER

__IM uint32_t CLR_RX_OVER

Clear RX_OVER Interrupt Register, Address offset: 0x048

## ◆ CLR_RX_UNDER

__IM uint32_t CLR_RX_UNDER

Clear RX_UNDER Interrupt Register, Address offset: 0x044

## ◆ CLR_SCL_STUCK_DET

__IM uint32_t CLR_SCL_STUCK_DET

Clear SCL Stuck at Low Detect Interrupt Register, Address offset: 0x0B4

## ◆ CLR_SMBUS_INTR

__OM uint32_t CLR_SMBUS_INTR

SMBus Clear Interrupt Register, Address offset: 0x0D4

## ◆ CLR_START_DET

__IM uint32_t CLR_START_DET

Clear START_DET Interrupt Register, Address offset: 0x064

## ◆ CLR_STOP_DET

__IM uint32_t CLR_STOP_DET

Clear STOP_DET Interrupt Register, Address offset: 0x060

## ◆ CLR_TX_ABRT

__IM uint32_t CLR_TX_ABRT

Clear TX_ABRT Interrupt Register, Address offset: 0x054

## ◆ CLR_TX_OVER

__IM uint32_t CLR_TX_OVER

Clear TX_OVER Interrupt Register, Address offset: 0x04C

## ◆ CON

__IOM uint32_t CON

I2C Control Register, Address offset: 0x000

## ◆ DATA_CMD

__IOM uint32_t DATA_CMD

I2C Rx/Tx Data Buffer and Command Register, Address offset: 0x010

## ◆ DMA_CR

__IOM uint32_t DMA_CR

DMA Control Register, Address offset: 0x088

## ◆ DMA_RDLR

__IOM uint32_t DMA_RDLR

DMA Receive Data Level Register, Address offset: 0x090

## ◆ DMA_TDLR

__IOM uint32_t DMA_TDLR

DMA Transmit Data Level Register, Address offset: 0x08C

## ◆ ENABLE

__IOM uint32_t ENABLE

I2C Enable Register, Address offset: 0x06C

## ◆ ENABLE_STATUS

__IM uint32_t ENABLE_STATUS

I2C Enable Status Register, Address offset: 0x09C

## ◆ FS_SCL_HCNT

__IOM uint32_t FS_SCL_HCNT

Fast Mode or Fast Mode Plus I2C Clock SCL High Count Register, Address offset: 0x01C

## ◆ FS_SCL_LCNT

__IOM uint32_t FS_SCL_LCNT

Fast Mode or Fast Mode Plus I2C Clock SCL Low Count Register, Address offset: 0x020

## ◆ FS_SPKLEN

__IOM uint32_t FS_SPKLEN

I2C SS, FS or FM+ spike suppression limit, Address offset: 0x0A0

## ◆ HS_MADDR

__IOM uint32_t HS_MADDR

I2C High Speed Master Mode Code Address Register, Address offset: 0x00C

## ◆ HS_SCL_HCNT

__IOM uint32_t HS_SCL_HCNT

High Speed I2C Clock SCL High Count Register, Address offset: 0x024

## ◆ HS_SCL_LCNT

__IOM uint32_t HS_SCL_LCNT

High Speed I2C Clock SCL Low Count Register, Address offset: 0x028

## ◆ HS_SPKLEN

__IOM uint32_t HS_SPKLEN

I2C HS spike suppression limit, Address offset: 0x0A4

## ◆ INTR_MASK

__IOM uint32_t INTR_MASK

I2C Interrupt Mask Register, Address offset: 0x030

## ◆ INTR_STAT

__IM uint32_t INTR_STAT

I2C Interrupt Status Register, Address offset: 0x02C

## ◆ OPTIONAL_SAR

__IOM uint32_t OPTIONAL_SAR

I2C Optional Slave Address Register, Address offset: 0x0D8

## ◆ RAW_INTR_STAT

__IM uint32_t RAW_INTR_STAT

I2C Raw Interrupt Status Register, Address offset: 0x034

## ◆ RESERVED0

uint32_t RESERVED0

Reserved, 0x0B8

## ◆ RX_TL

__IOM uint32_t RX_TL

I2C Receive FIFO Threshold Register, Address offset: 0x038

## ◆ RXFLR

__IM uint32_t RXFLR

I2C Receive FIFO Level Register, Address offset: 0x078

## ◆ SAR

__IOM uint32_t SAR

I2C Slave Address Register, Address offset: 0x008

## ◆ SCL_STUCK_AT_LOW_TIMEOUT

__IOM uint32_t SCL_STUCK_AT_LOW_TIMEOUT

I2C SCL Stuck at Low Timeout, Address offset: 0x0AC

## ◆ SDA_HOLD

__IOM uint32_t SDA_HOLD

I2C SDA Hold Time Length Register, Address offset: 0x07C

## ◆ SDA_SETUP

__IOM uint32_t SDA_SETUP

I2C SDA Setup Register, Address offset: 0x094

## ◆ SDA_STUCK_AT_LOW_TIMEOUT

__IOM uint32_t SDA_STUCK_AT_LOW_TIMEOUT

I2C SDA Stuck at Low Timeout, Address offset: 0x0B0

## ◆ SLV_DATA_NACK_ONLY

__IOM uint32_t SLV_DATA_NACK_ONLY

Generate Slave Data NACK Register, Address offset: 0x084

## ◆ SMBUS_CLK_LOW_MEXT

__IOM uint32_t SMBUS_CLK_LOW_MEXT

SMBus Master Clock Extend Timeout Register, Address offset: 0x0C0

## ◆ SMBUS_CLK_LOW_SEXT

__IOM uint32_t SMBUS_CLK_LOW_SEXT

SMBus Slave Clock Extend Timeout Register, Address offset: 0x0BC

## ◆ SMBUS_INTR_MASK

__IOM uint32_t SMBUS_INTR_MASK

SMBus Interrupt Mask Register, Address offset: 0x0CC

## ◆ SMBUS_INTR_STAT

__IM uint32_t SMBUS_INTR_STAT

SMBUS Interrupt Status Register, Address offset: 0x0C8

## ◆ SMBUS_RAW_INTR_STAT

__IM uint32_t SMBUS_RAW_INTR_STAT

SMBus Raw Interrupt Status Register, Address offset: 0x0D0

## ◆ SMBUS_THIGH_MAX_IDLE_COUNT

__IOM uint32_t SMBUS_THIGH_MAX_IDLE_COUNT

SMBus Master THigh MAX Bus-idle count Register, Address offset: 0x0C4

## ◆ SMBUS_UDID_LSB

__IOM uint32_t SMBUS_UDID_LSB

SMBUS ARP UDID LSB Register, Address offset: 0x0DC

## ◆ SS_SCL_HCNT

__IOM uint32_t SS_SCL_HCNT

Standard Speed I2C Clock SCL High Count Register, Address offset: 0x014

## ◆ SS_SCL_LCNT

__IOM uint32_t SS_SCL_LCNT

Standard Speed I2C Clock SCL Low Count Register, Address offset: 0x018

## ◆ STATUS

__IM uint32_t STATUS

I2C Status Register, Address offset: 0x070

## ◆ TAR

__IOM uint32_t TAR

I2C Target Address Register, Address offset: 0x004

## ◆ TX_ABRT_SOURCE

__IM uint32_t TX_ABRT_SOURCE

I2C Transmit Abort Source Register, Address offset: 0x080

## ◆ TX_TL

__IOM uint32_t TX_TL

I2C Transmit FIFO Threshold Register, Address offset: 0x03C

## ◆ TXFLR

__IM uint32_t TXFLR

I2C Transmit FIFO Level Register, Address offset: 0x074

该结构体的文档由以下文件生成:

- wb32f10x.h