WB32F10x Standard Peripherals Firmware Library

结构体 | 宏定义 | 函数
wb32f10x_adc.h 文件参考

This file contains all the functions prototypes for the ADC firmware library. 更多...

`#include "wb32f10x.h"`

浏览源代码.

## 结构体
struct | ADC_InitTypeDef
| ADC Init structure definition 更多...

## 宏定义
#define | ADC_ExternalTrigConv_T1_CC1 ((uint32_t)0x00000000)
#define | ADC_ExternalTrigConv_T1_CC2 ((uint32_t)0x00020000)
#define | ADC_ExternalTrigConv_T1_CC3 ((uint32_t)0x00040000)
#define | ADC_ExternalTrigConv_T2_CC2 ((uint32_t)0x00060000)
#define | ADC_ExternalTrigConv_T3_TRGO ((uint32_t)0x00080000)
#define | ADC_ExternalTrigConv_T4_CC4 ((uint32_t)0x000A0000)
#define | ADC_ExternalTrigConv_Ext_IT11 ((uint32_t)0x000C0000)
#define | ADC_ExternalTrigConv_None ((uint32_t)0x000E0000)
#define | IS_ADC_EXT_TRIG(REGTRIG)
#define | ADC_DataAlign_Right ((uint32_t)0x00000000)
#define | ADC_DataAlign_Left ((uint32_t)0x00000800)
#define | IS_ADC_DATA_ALIGN(ALIGN)
#define | ADC_Channel_0 ((uint8_t)0x00)
#define | ADC_Channel_1 ((uint8_t)0x01)
#define | ADC_Channel_2 ((uint8_t)0x02)
#define | ADC_Channel_3 ((uint8_t)0x03)
#define | ADC_Channel_4 ((uint8_t)0x04)
#define | ADC_Channel_5 ((uint8_t)0x05)
#define | ADC_Channel_6 ((uint8_t)0x06)
#define | ADC_Channel_7 ((uint8_t)0x07)
#define | ADC_Channel_8 ((uint8_t)0x08)
#define | ADC_Channel_9 ((uint8_t)0x09)
#define | ADC_Channel_10 ((uint8_t)0x0A)
#define | ADC_Channel_11 ((uint8_t)0x0B)
#define | ADC_Channel_12 ((uint8_t)0x0C)
#define | ADC_Channel_13 ((uint8_t)0x0D)
#define | ADC_Channel_14 ((uint8_t)0x0E)
#define | ADC_Channel_15 ((uint8_t)0x0F)
#define | ADC_Channel_16 ((uint8_t)0x10)
#define | ADC_Channel_17 ((uint8_t)0x11)
#define | ADC_Channel_TempSensor ((uint8_t)ADC_Channel_16)
#define | ADC_Channel_Vrefint ((uint8_t)ADC_Channel_17)
#define | IS_ADC_CHANNEL(CHANNEL)
#define | ADC_SampleTime_1Cycles5 ((uint8_t)0x00)
#define | ADC_SampleTime_7Cycles5 ((uint8_t)0x01)
#define | ADC_SampleTime_13Cycles5 ((uint8_t)0x02)
#define | ADC_SampleTime_28Cycles5 ((uint8_t)0x03)
#define | ADC_SampleTime_41Cycles5 ((uint8_t)0x04)
#define | ADC_SampleTime_55Cycles5 ((uint8_t)0x05)
#define | ADC_SampleTime_71Cycles5 ((uint8_t)0x06)
#define | ADC_SampleTime_239Cycles5 ((uint8_t)0x07)
#define | IS_ADC_SAMPLE_TIME(TIME)
#define | ADC_ExternalTrigInjecConv_T1_TRGO ((uint32_t)0x00000000)
#define | ADC_ExternalTrigInjecConv_T1_CC4 ((uint32_t)0x00001000)
#define | ADC_ExternalTrigInjecConv_T2_TRGO ((uint32_t)0x00002000)
#define | ADC_ExternalTrigInjecConv_T2_CC1 ((uint32_t)0x00003000)
#define | ADC_ExternalTrigInjecConv_T3_CC4 ((uint32_t)0x00004000)
#define | ADC_ExternalTrigInjecConv_T4_TRGO ((uint32_t)0x00005000)
#define | ADC_ExternalTrigInjecConv_Ext_IT15 ((uint32_t)0x00006000)
#define | ADC_ExternalTrigInjecConv_None ((uint32_t)0x00007000)
#define | IS_ADC_EXT_INJEC_TRIG(INJTRIG)
#define | ADC_InjectedChannel_1 ((uint8_t)0x14)
#define | ADC_InjectedChannel_2 ((uint8_t)0x18)
#define | ADC_InjectedChannel_3 ((uint8_t)0x1C)
#define | ADC_InjectedChannel_4 ((uint8_t)0x20)
#define | IS_ADC_INJECTED_CHANNEL(CHANNEL)
#define | ADC_AnalogWatchdog_SingleRegEnable ((uint32_t)0x00800200)
#define | ADC_AnalogWatchdog_SingleInjecEnable ((uint32_t)0x00400200)
#define | ADC_AnalogWatchdog_SingleRegOrInjecEnable ((uint32_t)0x00C00200)
#define | ADC_AnalogWatchdog_AllRegEnable ((uint32_t)0x00800000)
#define | ADC_AnalogWatchdog_AllInjecEnable ((uint32_t)0x00400000)
#define | ADC_AnalogWatchdog_AllRegAllInjecEnable ((uint32_t)0x00C00000)
#define | ADC_AnalogWatchdog_None ((uint32_t)0x00000000)
#define | IS_ADC_ANALOG_WATCHDOG(WATCHDOG)
#define | ADC_IT_EOC ((uint16_t)0x0220)
#define | ADC_IT_AWD ((uint16_t)0x0140)
#define | ADC_IT_JEOC ((uint16_t)0x0480)
#define | ADC_IT_OVF ((uint16_t)0x4001)
#define | ADC_IT_EMP ((uint16_t)0x2002)
#define | IS_ADC_IT(IT) ((((IT) & (uint16_t)0x981C) == 0x00) && ((IT) != 0x00))
#define | IS_ADC_GET_IT(IT)
#define | ADC_FLAG_AWD ((uint8_t)0x01)
#define | ADC_FLAG_EOC ((uint8_t)0x02)
#define | ADC_FLAG_JEOC ((uint8_t)0x04)
#define | ADC_FLAG_JSTRT ((uint8_t)0x08)
#define | ADC_FLAG_STRT ((uint8_t)0x10)
#define | ADC_FLAG_EMP ((uint8_t)0x20)
#define | ADC_FLAG_OVF ((uint8_t)0x40)
#define | IS_ADC_CLEAR_FLAG(FLAG) ((((FLAG) & (uint8_t)0xE0) == 0x00) && ((FLAG) != 0x00))
#define | IS_ADC_GET_FLAG(FLAG)
#define | IS_ADC_THRESHOLD(THRESHOLD) ((THRESHOLD) <= 0xFFF)
#define | IS_ADC_OFFSET(OFFSET) ((OFFSET) <= 0xFFF)
#define | IS_ADC_INJECTED_LENGTH(LENGTH) (((LENGTH) >= 0x1) && ((LENGTH) <= 0x4))
#define | IS_ADC_INJECTED_RANK(RANK) (((RANK) >= 0x1) && ((RANK) <= 0x4))
#define | IS_ADC_REGULAR_LENGTH(LENGTH) (((LENGTH) >= 0x1) && ((LENGTH) <= 0x10))
#define | IS_ADC_REGULAR_RANK(RANK) (((RANK) >= 0x1) && ((RANK) <= 0x10))
#define | IS_ADC_REGULAR_DISC_NUMBER(NUMBER) (((NUMBER) >= 0x1) && ((NUMBER) <= 0x8))

## 函数
void | ADC_DeInit (void)
| Deinitializes the ADC peripheral registers to their default reset values. 更多...
void | ADC_Init (ADC_InitTypeDef *ADC_InitStruct)
| Initializes the ADC peripheral according to the specified parameters in the ADC_InitStruct. 更多...
void | ADC_StructInit (ADC_InitTypeDef *ADC_InitStruct)
| Fills each ADC_InitStruct member with its default value. 更多...
void | ADC_Cmd (FunctionalState NewState)
| Enables or disables the ADC peripheral. 更多...
void | ADC_DMACmd (FunctionalState NewState)
| Enables or disables the ADC DMA request. 更多...
void | ADC_InjectedDMACmd (FunctionalState NewState)
| Enables or disables the ADC injected group DMA request. 更多...
void | ADC_ITConfig (uint16_t ADC_IT, FunctionalState NewState)
| Enables or disables the specified ADC interrupts. 更多...
void | ADC_ResetCalibration (void)
| Resets the selected ADC calibration registers. 更多...
FlagStatus | ADC_GetResetCalibrationStatus (void)
| Gets the selected ADC reset calibration registers status. 更多...
void | ADC_StartCalibration (void)
| Starts the selected ADC calibration process. 更多...
FlagStatus | ADC_GetCalibrationStatus (void)
| Gets the selected ADC calibration status. 更多...
void | ADC_SoftwareStartConvCmd (FunctionalState NewState)
| Enables or disables the selected ADC software start conversion . 更多...
FlagStatus | ADC_GetSoftwareStartConvStatus (void)
| Gets the selected ADC Software start conversion Status. 更多...
void | ADC_DiscModeChannelCountConfig (uint8_t Number)
| Configures the discontinuous mode for the selected ADC regular group channel. 更多...
void | ADC_DiscModeCmd (FunctionalState NewState)
| Enables or disables the discontinuous mode on regular group channel for the ADC 更多...
void | ADC_RegularChannelConfig (uint8_t ADC_Channel, uint8_t Rank, uint8_t ADC_SampleTime)
| Configures for the selected ADC regular channel its corresponding rank in the sequencer and its sample time. 更多...
void | ADC_ExternalTrigConvCmd (FunctionalState NewState)
| Enables or disables the ADC conversion through external trigger. 更多...
uint16_t | ADC_GetConversionValue (void)
| Returns the last ADC conversion result data for regular channel. 更多...
void | ADC_AutoInjectedConvCmd (FunctionalState NewState)
| Enables or disables the selected ADC automatic injected group conversion after regular one. 更多...
void | ADC_InjectedDiscModeCmd (FunctionalState NewState)
| Enables or disables the discontinuous mode for injected group channel for the ADC 更多...
void | ADC_ExternalTrigInjectedConvConfig (uint32_t ADC_ExternalTrigInjecConv)
| Configures the ADC external trigger for injected channels conversion. 更多...
void | ADC_ExternalTrigInjectedConvCmd (FunctionalState NewState)
| Enables or disables the ADC injected channels conversion through external trigger 更多...
void | ADC_SoftwareStartInjectedConvCmd (FunctionalState NewState)
| Enables or disables the selected ADC start of the injected channels conversion. 更多...
FlagStatus | ADC_GetSoftwareStartInjectedConvCmdStatus (void)
| Gets the selected ADC Software start injected conversion Status. 更多...
void | ADC_InjectedChannelConfig (uint8_t ADC_Channel, uint8_t Rank, uint8_t ADC_SampleTime)
| Configures for the selected ADC injected channel its corresponding rank in the sequencer and its sample time. 更多...
void | ADC_InjectedSequencerLengthConfig (uint8_t Length)
| Configures the sequencer length for injected channels 更多...
void | ADC_SetInjectedOffset (uint8_t ADC_InjectedChannel, uint16_t Offset)
| Set the injected channels conversion value offset 更多...
uint16_t | ADC_GetInjectedConversionValue (uint8_t ADC_InjectedChannel)
| Returns the ADC injected channel conversion result 更多...
void | ADC_AnalogWatchdogCmd (uint32_t ADC_AnalogWatchdog)
| Enables or disables the analog watchdog on single/all regular or injected channels 更多...
void | ADC_AnalogWatchdogThresholdsConfig (uint16_t HighThreshold, uint16_t LowThreshold)
| Configures the high and low thresholds of the analog watchdog. 更多...
void | ADC_AnalogWatchdogSingleChannelConfig (uint8_t ADC_Channel)
| Configures the analog watchdog guarded single channel 更多...
void | ADC_TempSensorVrefintCmd (FunctionalState NewState)
| Enables or disables the temperature sensor and Vrefint channel. 更多...
FlagStatus | ADC_GetFlagStatus (uint8_t ADC_FLAG)
| Checks whether the specified ADC flag is set or not. 更多...
void | ADC_ClearFlag (uint8_t ADC_FLAG)
| Clears the ADC's pending flags. 更多...
ITStatus | ADC_GetITStatus (uint16_t ADC_IT)
| Checks whether the specified ADC interrupt has occurred or not. 更多...
void | ADC_ClearITPendingBit (uint16_t ADC_IT)
| Clears the ADC's interrupt pending bits. 更多...
uint16_t | ADC_GetADValue (uint16_t data)
| Adjust the ADC conversion result. 更多...

## 详细描述

This file contains all the functions prototypes for the ADC firmware library.

作者
  Westberry Application Team

版本
  V0.1.10

日期
  05-January-2023