WB32F10x Standard Peripherals Firmware Library

Data Fields
APSR_Type Union Reference
Defines and Type Definitions » Status and Control Registers

Union type to access the Application Program Status Register (APSR). More...

`#include <core_cm3.h>`

## Data Fields
struct {
uint32_t _reserved0:27
uint32_t Q:1
uint32_t V:1
uint32_t C:1
uint32_t Z:1
uint32_t N:1
} | b
uint32_t | w

## Detailed Description

Union type to access the Application Program Status Register (APSR).

## Field Documentation

## ◆ _reserved0

uint32_t _reserved0

bit: 0..26 Reserved

## ◆ b

struct { ... } b

Structure used for bit access

## ◆ C

uint32_t C

bit: 29 Carry condition code flag

## ◆ N

uint32_t N

bit: 31 Negative condition code flag

## ◆ Q

uint32_t Q

bit: 27 Saturation condition flag

## ◆ V

uint32_t V

bit: 28 Overflow condition code flag

## ◆ w

uint32_t w

Type used for word access

## ◆ Z

uint32_t Z

bit: 30 Zero condition code flag

The documentation for this union was generated from the following file:

- core_cm3.h