WB32F10x Standard Peripherals Firmware Library

SysTick_Example example

      *************** (C) COPYRIGHT 2020 - 2023 Westberry Technology ***************
      * @file    SysTick/SysTick_Example/readme.txt
      * @author  Westberry Application Team
      * @version V0.1.10
      * @date    05-January-2023
      * @brief   Description of the SysTick SysTick_Example example.
      ******************************************************************************
      * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
      * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
      * TIME. AS A RESULT, WESTBERRY SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
      * INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM
      * THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
      * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
      ******************************************************************************

例程描述

本例程演示如何配置SysTick以生成1ms的时基。

本例程系统时钟工作在96Mhz，通过PLL配置产生。PLL时钟源是外部8Mhz晶振。APB1的分频比是1，APB2的分频比是1。

目录内容

- SysTick/SysTick_Example/SysTick_Example.uvprojx MDK5工程文件
- SysTick/SysTick_Example/SysTick_Example.uvoptx MDK5工程配置文件
- SysTick/SysTick_Example/JLinkSettings.ini Jlink配置文件
- SysTick/SysTick_Example/main.c 主程序

硬件和软件环境

- 硬件平台搭建
  - HSE 连接外部8MHz晶振

如何使用？

为了使程序工作，您必须执行以下操作 :

- 使用 MDK5 打开此例程文件夹中的 SysTick_Example.uvprojx 工程
- 重新编译该工程并下载到目标存储器中

- 运行此例程

  ###
  © COPYRIGHT 2020 - 2023 Westberry Technology