WB32F10x Standard Peripherals Firmware Library

IWDG_Reset example

      *************** (C) COPYRIGHT 2020 - 2023 Westberry Technology ***************
      * @file    IWDG/IWDG_Reset/readme.txt
      * @author  Westberry Application Team
      * @version V0.1.10
      * @date    05-January-2023
      * @brief   Description of the IWDG IWDG_Reset example.
      ******************************************************************************
      * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
      * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
      * TIME. AS A RESULT, WESTBERRY SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
      * INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM
      * THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
      * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
      ******************************************************************************

例程描述

本例程演示如何使用IWDG。

本例程系统时钟工作在96Mhz，通过PLL配置产生。PLL时钟源是外部8Mhz晶振。APB1的分频比是1，APB2的分频比是1。

需要注意目前IWDG存在的一些限制：
1, 一旦启用了IWDG，即使发生复位也无法禁用它。
解决方法：在程序运行之前将IWDG超时设置配置为最大，并且之后要不断重载IWDG计数器。

2, 如果IWDG启动之后发生复位，那么IWDG域需要3个LSI时钟周期才能就绪。
解决方法：在LSI就绪后，配置IWDG之前，等待大概1毫秒。

3, 不断执行IWDG reload counter操作有几率无法reload IWDG counter.
解决方法：在执行reload IWDG counter操作之前确保RVU位是0。（RVU位指示reload counter操作是否完成，）

目录内容

- IWDG/IWDG_Reset/IWDG_Reset.uvprojx MDK5工程文件
- IWDG/IWDG_Reset/IWDG_Reset.uvoptx MDK5工程配置文件
- IWDG/IWDG_Reset/JLinkSettings.ini Jlink配置文件
- IWDG/IWDG_Reset/main.c 主程序

硬件和软件环境

- 硬件平台搭建
  - HSE 连接外部8MHz晶振

如何使用？

为了使程序工作，您必须执行以下操作 :

- 使用 MDK5 打开此例程文件夹中的 IWDG_Reset.uvprojx 工程
- 重新编译该工程并下载到目标存储器中

- 运行此例程

  ###
  © COPYRIGHT 2020 - 2023 Westberry Technology