WB32F10x Standard Peripherals Firmware Library

PWR_STOP example

      *************** (C) COPYRIGHT 2020 - 2023 Westberry Technology ***************
      * @file    PWR/PWR_STOP/readme.txt
      * @author  Westberry Application Team
      * @version V0.1.10
      * @date    05-January-2023
      * @brief   Description of the PWR PWR_STOP example.
      ******************************************************************************
      * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
      * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
      * TIME. AS A RESULT, WESTBERRY SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
      * INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM
      * THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
      * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
      ******************************************************************************

例程描述

本例程演示如何进入低功耗STOP模式和通过外部中断退出低功耗STOP模式。

本例程执行以下操作：

1. 打开HSE，HSE作为PLL的时钟源，PLL倍频到96MHz，PLL时钟作为主时钟。
2. 点亮LED1，熄灭LED2。
3. 等待一段时间后，配置PA0上升沿中断并进入低功耗STOP模式。
4. 此时处于低功耗STOP模式。按下与PA0连接的按键产生EXTI0中断以唤醒芯片。
5. 在EXTI0中断中，切换LED2的状态（LED2点亮）。
6. 由于在进入低功耗STOP模式时关闭了一些时钟配置，所以退出低功耗STOP模式后重新配置相关时钟。
7. LED1闪烁。

目录内容

- PWR/PWR_STOP/PWR_STOP.uvprojx MDK5工程文件
- PWR/PWR_STOP/PWR_STOP.uvoptx MDK5工程配置文件
- PWR/PWR_STOP/JLinkSettings.ini Jlink配置文件
- PWR/PWR_STOP/main.c 主程序

硬件和软件环境

- 硬件平台搭建
  - HSE 连接外部8MHz晶振
  - 芯片管脚连接如下：
    - PB14 管脚连接到 LED1
    - PB13 管脚连接到 LED2
    - PA0 管脚连接到按键

如何使用？

为了使程序工作，您必须执行以下操作 :

- 使用 MDK5 打开此例程文件夹中的 PWR_STOP.uvprojx 工程
- 重新编译该工程并下载到目标存储器中

- 运行此例程

  ###
  © COPYRIGHT 2020 - 2023 Westberry Technology