WB32F10x Standard Peripherals Firmware Library

宏定义 | 枚举 | 函数
wb32f10x_gpio.h 文件参考

This file contains all the functions prototypes for the GPIO firmware library. 更多...

`#include "wb32f10x.h"`

浏览源代码.

## 宏定义
#define | IS_GPIO_ALL_PERIPH(PERIPH)
#define | IS_GPIO_BIT_ACTION(ACTION) (((ACTION) == Bit_RESET) || ((ACTION) == Bit_SET))
#define | GPIO_Pin_0 ((uint16_t)0x0001)
#define | GPIO_Pin_1 ((uint16_t)0x0002)
#define | GPIO_Pin_2 ((uint16_t)0x0004)
#define | GPIO_Pin_3 ((uint16_t)0x0008)
#define | GPIO_Pin_4 ((uint16_t)0x0010)
#define | GPIO_Pin_5 ((uint16_t)0x0020)
#define | GPIO_Pin_6 ((uint16_t)0x0040)
#define | GPIO_Pin_7 ((uint16_t)0x0080)
#define | GPIO_Pin_8 ((uint16_t)0x0100)
#define | GPIO_Pin_9 ((uint16_t)0x0200)
#define | GPIO_Pin_10 ((uint16_t)0x0400)
#define | GPIO_Pin_11 ((uint16_t)0x0800)
#define | GPIO_Pin_12 ((uint16_t)0x1000)
#define | GPIO_Pin_13 ((uint16_t)0x2000)
#define | GPIO_Pin_14 ((uint16_t)0x4000)
#define | GPIO_Pin_15 ((uint16_t)0x8000)
#define | GPIO_Pin_All ((uint16_t)0xFFFF)
#define | IS_GPIO_PIN(PIN) (((PIN) & 0x0000FFFF) != (uint32_t)0x00)
#define | IS_GET_GPIO_PIN(PIN)
#define | GPIO_PortSourceGPIOA ((uint8_t)0x00)
#define | GPIO_PortSourceGPIOB ((uint8_t)0x01)
#define | GPIO_PortSourceGPIOC ((uint8_t)0x02)
#define | GPIO_PortSourceGPIOD ((uint8_t)0x03)
#define | GPIO_PinSource0 ((uint8_t)0x00)
#define | GPIO_PinSource1 ((uint8_t)0x01)
#define | GPIO_PinSource2 ((uint8_t)0x02)
#define | GPIO_PinSource3 ((uint8_t)0x03)
#define | GPIO_PinSource4 ((uint8_t)0x04)
#define | GPIO_PinSource5 ((uint8_t)0x05)
#define | GPIO_PinSource6 ((uint8_t)0x06)
#define | GPIO_PinSource7 ((uint8_t)0x07)
#define | GPIO_PinSource8 ((uint8_t)0x08)
#define | GPIO_PinSource9 ((uint8_t)0x09)
#define | GPIO_PinSource10 ((uint8_t)0x0A)
#define | GPIO_PinSource11 ((uint8_t)0x0B)
#define | GPIO_PinSource12 ((uint8_t)0x0C)
#define | GPIO_PinSource13 ((uint8_t)0x0D)
#define | GPIO_PinSource14 ((uint8_t)0x0E)
#define | GPIO_PinSource15 ((uint8_t)0x0F)
#define | IS_GPIO_PIN_SOURCE(PINSOURCE)
#define | GPIO_MODE_IN 0x00000000U
#define | GPIO_MODE_OUT 0x10000000U
#define | GPIO_MODE_AF 0x20000000U
#define | GPIO_MODE_ANA 0x30000000U
#define | GPIO_OTYPE_PP 0x00000000U
#define | GPIO_OTYPE_OD 0x01000000U
#define | GPIO_SPEED_LOW 0x00100000U
#define | GPIO_SPEED_HIGH 0x00000000U
#define | GPIO_PUPD_NOPULL 0x00000000U
#define | GPIO_PUPD_UP 0x00010000U
#define | GPIO_PUPD_DOWN 0x00020000U
#define | GPIO_AF0 0
#define | GPIO_AF1 1
#define | GPIO_AF2 2
#define | GPIO_AF3 3
#define | GPIO_AF4 4
#define | GPIO_AF5 5
#define | GPIO_AF6 6
#define | GPIO_AF7 7
#define | GPIO_AF8 8
#define | GPIO_AF9 9
#define | GPIO_AF10 10
#define | GPIO_AF11 11
#define | GPIO_AF12 12
#define | GPIO_AF13 13
#define | GPIO_AF14 14
#define | GPIO_AF15 15

## 枚举
enum | BitAction { Bit_RESET = 0, Bit_SET }
| GPIO Bit SET and Bit RESET enumeration

## 函数
void | GPIO_DeInit (GPIO_TypeDef *GPIOx)
| De-initializes the GPIOx peripheral registers to their default reset values. 更多...
void | GPIO_Init (GPIO_TypeDef *GPIOx, uint16_t GPIO_Pin, uint32_t PinConfig)
| Initializes the GPIOx peripheral according to the PinConfig. 更多...
void | GPIO_SetAFPin_0_7 (GPIO_TypeDef *GPIOx, uint16_t GPIO_Pin, uint32_t Alternate)
| Configure gpio alternate function of a dedicated pin from 0 to 7 for a dedicated port. 更多...
void | GPIO_SetAFPin_8_15 (GPIO_TypeDef *GPIOx, uint16_t GPIO_Pin, uint32_t Alternate)
| Configure gpio alternate function of a dedicated pin from 8 to 15 for a dedicated port. 更多...
void | GPIO_SetAFPin (GPIO_TypeDef *GPIOx, uint16_t GPIO_Pin, uint32_t Alternate)
| Configure gpio alternate function of any pins for a dedicated port. 更多...
uint8_t | GPIO_ReadInputDataBit (GPIO_TypeDef *GPIOx, uint16_t GPIO_Pin)
| Reads the specified input port pin. 更多...
uint16_t | GPIO_ReadInputData (GPIO_TypeDef *GPIOx)
| Reads the specified GPIO input data port. 更多...
uint8_t | GPIO_ReadOutputDataBit (GPIO_TypeDef *GPIOx, uint16_t GPIO_Pin)
| Reads the specified output data port bit. 更多...
uint16_t | GPIO_ReadOutputData (GPIO_TypeDef *GPIOx)
| Reads the specified GPIO output data port. 更多...
void | GPIO_SetBits (GPIO_TypeDef *GPIOx, uint16_t GPIO_Pin)
| Sets the selected data port bits. 更多...
void | GPIO_ResetBits (GPIO_TypeDef *GPIOx, uint16_t GPIO_Pin)
| Clears the selected data port bits. 更多...
void | GPIO_WriteBit (GPIO_TypeDef *GPIOx, uint16_t GPIO_Pin, BitAction BitVal)
| Sets or clears the selected data port bit. 更多...
void | GPIO_Write (GPIO_TypeDef *GPIOx, uint16_t PortVal)
| Writes data to the specified GPIO data port. 更多...
void | GPIO_ToggleBits (GPIO_TypeDef *GPIOx, uint16_t GPIO_Pin)
| Toggle data value for several pin of specified port. 更多...
void | GPIO_LockPin (GPIO_TypeDef *GPIOx, uint16_t GPIO_Pin)
| Lock configuration of several pins for a specified port. 更多...
uint32_t | GPIO_IsPinLocked (GPIO_TypeDef *GPIOx, uint16_t GPIO_Pin)
| Return 1 if all pins passed as parameter, of a specified port, are locked. else Return 0. 更多...
void | GPIO_SchmittTriggerCmd (GPIO_TypeDef *GPIOx, uint16_t GPIO_Pin, FunctionalState NewState)
| Enables or disables the schmitt trigger of several pins for a specified port. 更多...
void | GPIO_DriveCurrentConfig (GPIO_TypeDef *GPIOx, uint16_t GPIO_Pin, uint32_t Current)
| Configure the drive current of several pins for a specified port. 更多...
void | GPIO_EXTILineConfig (uint8_t GPIO_PortSource, uint8_t GPIO_PinSource)
| Selects the GPIO pin used as EXTI Line. 更多...

## 详细描述

This file contains all the functions prototypes for the GPIO firmware library.

作者
  Westberry Application Team

版本
  V0.1.10

日期
  05-January-2023