WB32F10x Standard Peripherals Firmware Library

Data Fields
UART_InitTypeDef Struct Reference
WB32F10x_StdPeriph_Driver » UART

UART Init Structure definition. More...

`#include <wb32f10x_uart.h>`

## Data Fields
uint32_t | UART_BaudRate
uint8_t | UART_WordLength
uint8_t | UART_StopBits
uint8_t | UART_Parity
uint8_t | UART_AutoFlowControl

## Detailed Description

UART Init Structure definition.

## Field Documentation

## ◆ UART_AutoFlowControl

uint8_t UART_AutoFlowControl

Specifies the auto flow control mode is enabled or disabled. This parameter can be a value of UART_AutoFlowControl example

## ◆ UART_BaudRate

uint32_t UART_BaudRate

This member configures the UART communication baud rate.

## ◆ UART_Parity

uint8_t UART_Parity

Specifies the parity mode. This parameter can be a value of UART_Parity

## ◆ UART_StopBits

uint8_t UART_StopBits

Specifies the number of stop bits transmitted. This parameter can be a value of UART_Stop_Bits

## ◆ UART_WordLength

uint8_t UART_WordLength

Specifies the number of data bits transmitted or received in a frame. This parameter can be a value of UART_Word_Length

The documentation for this struct was generated from the following file:

- wb32f10x_uart.h