WB32F10x Standard Peripherals Firmware Library

wb32f10x_i2c.h
浏览该文件的文档.
1
10 /* Define to prevent recursive inclusion -------------------------------------*/
11 #ifndef __WB32F10x_I2C_H
12 #define __WB32F10x_I2C_H
13
14 #ifdef __cplusplus
15 extern "C" {
16 #endif
17
18 /* Includes ------------------------------------------------------------------*/
19 #include "wb32f10x.h"
20
29 /* Exported types ------------------------------------------------------------*/
30 /* Exported constants --------------------------------------------------------*/
31
39 #define I2C_TARGETADDRESS_GENERAL_CALL (I2C_TAR_SPECIAL)
40 #define I2C_TARGETADDRESS_START_BYTE (I2C_TAR_SPECIAL | I2C_TAR_GC_OR_START)
41 #define I2C_TARGETADDRESS_DEVICE_ID (I2C_TAR_SPECIAL | I2C_TAR_DEVICE_ID)
42 #define I2C_TARGETADDRESS_SMBUS_QUICK_CMD (I2C_TAR_SPECIAL | I2C_TAR_SMBUS_QUICK_CMD)
43
51 #define I2C_FLAG_ACTIVITY I2C_STATUS_ACTIVITY
52 #define I2C_FLAG_TFNF I2C_STATUS_TFNF
53 #define I2C_FLAG_TFE I2C_STATUS_TFE
54 #define I2C_FLAG_RFNE I2C_STATUS_RFNE
55 #define I2C_FLAG_RFF I2C_STATUS_RFF
56 #define I2C_FLAG_MST_ACTIVITY I2C_STATUS_MST_ACTIVITY
57 #define I2C_FLAG_SLV_ACTIVITY I2C_STATUS_SLV_ACTIVITY
58 #define I2C_FLAG_MST_HOLD_TX_FIFO_EMPTY I2C_STATUS_MST_HOLD_TX_FIFO_EMPTY
59 #define I2C_FLAG_MST_HOLD_RX_FIFO_FULL I2C_STATUS_MST_HOLD_RX_FIFO_FULL
60 #define I2C_FLAG_SLV_HOLD_TX_FIFO_EMPTY I2C_STATUS_SLV_HOLD_TX_FIFO_EMPTY
61 #define I2C_FLAG_SLV_HOLD_RX_FIFO_FULL I2C_STATUS_SLV_HOLD_RX_FIFO_FULL
62 #define I2C_FLAG_SDA_STUCK_NOT_RECOVERED I2C_STATUS_SDA_STUCK_NOT_RECOVERED
63 #define I2C_FLAG_SMBUS_QUICK_CMD_BIT I2C_STATUS_SMBUS_QUICK_CMD_BIT
64 #define I2C_FLAG_SMBUS_SLAVE_ADDR_VALID I2C_STATUS_SMBUS_SLAVE_ADDR_VALID
65 #define I2C_FLAG_SMBUS_SLAVE_ADDR_RESOLVED I2C_STATUS_SMBUS_SLAVE_ADDR_RESOLVED
66 #define I2C_FLAG_SMBUS_SUSPEND_STATUS I2C_STATUS_SMBUS_SUSPEND_STATUS
67 #define I2C_FLAG_SMBUS_ALERT_STATUS I2C_STATUS_SMBUS_ALERT_STATUS
68
76 #define I2C_IT_RX_UNDER I2C_INTR_RX_UNDER
77 #define I2C_IT_RX_OVER I2C_INTR_RX_OVER
78 #define I2C_IT_RX_FULL I2C_INTR_RX_FULL
79 #define I2C_IT_TX_OVER I2C_INTR_TX_OVER
80 #define I2C_IT_TX_EMPTY I2C_INTR_TX_EMPTY
81 #define I2C_IT_RD_REQ I2C_INTR_RD_REQ
82 #define I2C_IT_TX_ABRT I2C_INTR_TX_ABRT
83 #define I2C_IT_RX_DONE I2C_INTR_RX_DONE
84 #define I2C_IT_ACTIVITY I2C_INTR_ACTIVITY
85 #define I2C_IT_STOP_DET I2C_INTR_STOP_DET
86 #define I2C_IT_START_DET I2C_INTR_START_DET
87 #define I2C_IT_GEN_CALL I2C_INTR_GEN_CALL
88 #define I2C_IT_RESTART_DET I2C_INTR_RESTART_DET
89 #define I2C_IT_SCL_STUCK_AT_LOW I2C_INTR_SCL_STUCK_AT_LOW
90
98 #define I2C_SMBUS_IT_SLV_CLOCK_EXTND_TIMEOUT I2C_SMBUS_INTR_SLV_CLOCK_EXTND_TIMEOUT
99 #define I2C_SMBUS_IT_MST_CLOCK_EXTND_TIMEOUT I2C_SMBUS_INTR_MST_CLOCK_EXTND_TIMEOUT
100 #define I2C_SMBUS_IT_QUICK_CMD_DET I2C_SMBUS_INTR_QUICK_CMD_DET
101 #define I2C_SMBUS_IT_HOST_NTFY_MST_DET I2C_SMBUS_INTR_HOST_NTFY_MST_DET
102 #define I2C_SMBUS_IT_ARP_PREPARE_CMD_DET I2C_SMBUS_INTR_ARP_PREPARE_CMD_DET
103 #define I2C_SMBUS_IT_ARP_RST_CMD_DET I2C_SMBUS_INTR_ARP_RST_CMD_DET
104 #define I2C_SMBUS_IT_ARP_GET_UDID_CMD_DET I2C_SMBUS_INTR_ARP_GET_UDID_CMD_DET
105 #define I2C_SMBUS_IT_ARP_ASSGN_ADDR_CMD_DET I2C_SMBUS_INTR_ARP_ASSGN_ADDR_CMD_DET
106 #define I2C_SMBUS_IT_SLV_RX_PEC_NACK I2C_SMBUS_INTR_SLV_RX_PEC_NACK
107 #define I2C_SMBUS_IT_SMBUS_SUSPEND_DET I2C_SMBUS_INTR_SMBUS_SUSPEND_DET
108 #define I2C_SMBUS_IT_SMBUS_ALERT_DET I2C_SMBUS_INTR_SMBUS_ALERT_DET
109
117 #define I2C_DMAReq_Rx I2C_DMA_CR_RDMAE
118 #define I2C_DMAReq_Tx I2C_DMA_CR_TDMAE
119
127 /* Exported macro ------------------------------------------------------------*/
128 /* Exported functions --------------------------------------------------------*/
129
130 void I2C_DeInit(I2C_TypeDef* I2Cx);
131 void I2C_Init(I2C_TypeDef* I2Cx, uint32_t I2C_CON);
132 void I2C_TargetAddressConfig(I2C_TypeDef* I2Cx, uint32_t TargetAddress);
133 void I2C_OwnAddressConfig(I2C_TypeDef* I2Cx, uint16_t Address);
134 void I2C_HighSpeedModeMasterCodeConfig(I2C_TypeDef* I2Cx, uint8_t Code);
135 uint32_t I2C_GetTxAbortSource(I2C_TypeDef* I2Cx);
136 void I2C_SCLStuckAtLowTimeoutConfig(I2C_TypeDef* I2Cx, uint32_t Timeout);
137 void I2C_SDAStuckAtLowTimeoutConfig(I2C_TypeDef* I2Cx, uint32_t Timeout);
138 void I2C_Cmd(I2C_TypeDef* I2Cx, FunctionalState NewState);
139 void I2C_SlaveDataNAckOnlyConfig(I2C_TypeDef* I2Cx, FunctionalState NewState);
140 void I2C_AckGeneralCallCmd(I2C_TypeDef* I2Cx, FunctionalState NewState);
141 uint16_t I2C_ReadData(I2C_TypeDef* I2Cx);
142 void I2C_WriteDataCmd(I2C_TypeDef* I2Cx, uint16_t I2C_DataCmd);
143 FlagStatus I2C_GetFlagStatus(I2C_TypeDef* I2Cx, uint32_t I2C_FLAG);
144 void I2C_ITConfig(I2C_TypeDef* I2Cx, uint16_t I2C_IT, FunctionalState NewState);
145 ITStatus I2C_GetRawITStatus(I2C_TypeDef* I2Cx, uint16_t I2C_IT);
146 ITStatus I2C_GetITStatus(I2C_TypeDef* I2Cx, uint16_t I2C_IT);
147 void I2C_ClearITPendingBit(I2C_TypeDef* I2Cx, uint16_t I2C_IT);
148 void I2C_RxFIFOThresholdConfig(I2C_TypeDef* I2Cx, uint8_t Threshold);
149 void I2C_TxFIFOThresholdConfig(I2C_TypeDef* I2Cx, uint8_t Threshold);
150 uint8_t I2C_GetRxFIFOLevel(I2C_TypeDef* I2Cx);
151 uint8_t I2C_GetTxFIFOLevel(I2C_TypeDef* I2Cx);
152 void I2C_DMARxReqLevelConfig(I2C_TypeDef* I2Cx, uint8_t Level);
153 void I2C_DMATxReqLevelConfig(I2C_TypeDef* I2Cx, uint8_t Level);
154 void I2C_DMACmd(I2C_TypeDef* I2Cx, uint32_t I2C_DMAReq, FunctionalState NewState);
155 void I2C_SMBus_ITConfig(I2C_TypeDef* I2Cx, uint16_t I2C_SMBUS_IT, FunctionalState NewState);
156 ITStatus I2C_SMBus_GetRawITStatus(I2C_TypeDef* I2Cx, uint16_t I2C_SMBUS_IT);
157 ITStatus I2C_SMBus_GetITStatus(I2C_TypeDef* I2Cx, uint16_t I2C_SMBUS_IT);
158 void I2C_SMBus_ClearITPendingBit(I2C_TypeDef* I2Cx, uint16_t I2C_SMBUS_IT);
159
168 #ifdef __cplusplus
169 }
170 #endif
171
172 #endif /* __WB32F10x_I2C_H */
I2C_Init
void I2C_Init(I2C_TypeDef *I2Cx, uint32_t I2C_CON)
Initializes the I2Cx peripheral according to the specified parameters in the I2C_InitStruct.
Definition: wb32f10x_i2c.c:64
I2C_RxFIFOThresholdConfig
void I2C_RxFIFOThresholdConfig(I2C_TypeDef *I2Cx, uint8_t Threshold)
Configures the Receive FIFO threshold.
Definition: wb32f10x_i2c.c:457
I2C_DMATxReqLevelConfig
void I2C_DMATxReqLevelConfig(I2C_TypeDef *I2Cx, uint8_t Level)
Configures the DMA Tx request level.
Definition: wb32f10x_i2c.c:521
I2C_WriteDataCmd
void I2C_WriteDataCmd(I2C_TypeDef *I2Cx, uint16_t I2C_DataCmd)
Write data and command Tx FIFO.
Definition: wb32f10x_i2c.c:224
I2C_GetRxFIFOLevel
uint8_t I2C_GetRxFIFOLevel(I2C_TypeDef *I2Cx)
Returns the number of valid data entries in the receive FIFO buffer.
Definition: wb32f10x_i2c.c:483
I2C_TxFIFOThresholdConfig
void I2C_TxFIFOThresholdConfig(I2C_TypeDef *I2Cx, uint8_t Threshold)
Configures the Transmit FIFO threshold.
Definition: wb32f10x_i2c.c:471
I2C_SlaveDataNAckOnlyConfig
void I2C_SlaveDataNAckOnlyConfig(I2C_TypeDef *I2Cx, FunctionalState NewState)
Enables or disables generate NACK after data byte received when as slave-receiver.
Definition: wb32f10x_i2c.c:175
I2C_GetRawITStatus
ITStatus I2C_GetRawITStatus(I2C_TypeDef *I2Cx, uint16_t I2C_IT)
Checks whether the specified I2Cx raw interrupt status.
Definition: wb32f10x_i2c.c:336
I2C_OwnAddressConfig
void I2C_OwnAddressConfig(I2C_TypeDef *I2Cx, uint16_t Address)
Configures the specified I2C own address.
Definition: wb32f10x_i2c.c:90
I2C_SCLStuckAtLowTimeoutConfig
void I2C_SCLStuckAtLowTimeoutConfig(I2C_TypeDef *I2Cx, uint32_t Timeout)
Configures the specified I2C SCL stuck at low timeout.
Definition: wb32f10x_i2c.c:128
I2C_SMBus_ITConfig
void I2C_SMBus_ITConfig(I2C_TypeDef *I2Cx, uint16_t I2C_SMBUS_IT, FunctionalState NewState)
Enables or disables the specified SMBus interrupts.
Definition: wb32f10x_i2c.c:571
I2C_DeInit
void I2C_DeInit(I2C_TypeDef *I2Cx)
Deinitializes the I2Cx peripheral registers to their default reset values.
Definition: wb32f10x_i2c.c:40
I2C_ClearITPendingBit
void I2C_ClearITPendingBit(I2C_TypeDef *I2Cx, uint16_t I2C_IT)
Clears the I2Cx's interrupt pending bits.
Definition: wb32f10x_i2c.c:418
I2C_Cmd
void I2C_Cmd(I2C_TypeDef *I2Cx, FunctionalState NewState)
Enables or disables the specified I2C peripheral.
Definition: wb32f10x_i2c.c:155
I2C_SMBus_ClearITPendingBit
void I2C_SMBus_ClearITPendingBit(I2C_TypeDef *I2Cx, uint16_t I2C_SMBUS_IT)
Clears the I2Cx's interrupt pending bits.
Definition: wb32f10x_i2c.c:683
I2C_GetFlagStatus
FlagStatus I2C_GetFlagStatus(I2C_TypeDef *I2Cx, uint32_t I2C_FLAG)
Checks whether the specified I2C flag is set or not.
Definition: wb32f10x_i2c.c:255
I2C_SMBus_GetITStatus
ITStatus I2C_SMBus_GetITStatus(I2C_TypeDef *I2Cx, uint16_t I2C_SMBUS_IT)
Checks whether the specified SMBus interrupt has occurred or not.
Definition: wb32f10x_i2c.c:644
I2C_AckGeneralCallCmd
void I2C_AckGeneralCallCmd(I2C_TypeDef *I2Cx, FunctionalState NewState)
Enables or disables the General Call ACK Generate.
Definition: wb32f10x_i2c.c:194
I2C_TargetAddressConfig
void I2C_TargetAddressConfig(I2C_TypeDef *I2Cx, uint32_t TargetAddress)
Configures the specified I2C target address.
Definition: wb32f10x_i2c.c:77
I2C_GetITStatus
ITStatus I2C_GetITStatus(I2C_TypeDef *I2Cx, uint16_t I2C_IT)
Checks whether the specified I2Cx interrupt has occurred or not.
Definition: wb32f10x_i2c.c:378
I2C_ITConfig
void I2C_ITConfig(I2C_TypeDef *I2Cx, uint16_t I2C_IT, FunctionalState NewState)
Enables or disables the specified I2C interrupts.
Definition: wb32f10x_i2c.c:299
I2C_GetTxFIFOLevel
uint8_t I2C_GetTxFIFOLevel(I2C_TypeDef *I2Cx)
Returns the number of valid data entries in the transmit FIFO buffer.
Definition: wb32f10x_i2c.c:495
I2C_TypeDef
Definition: wb32f10x.h:606
I2C_HighSpeedModeMasterCodeConfig
void I2C_HighSpeedModeMasterCodeConfig(I2C_TypeDef *I2Cx, uint8_t Code)
Configures the I2C HS mode master code.
Definition: wb32f10x_i2c.c:103
I2C_GetTxAbortSource
uint32_t I2C_GetTxAbortSource(I2C_TypeDef *I2Cx)
Returns the transmit abort source for the specified I2C.
Definition: wb32f10x_i2c.c:115
I2C_SDAStuckAtLowTimeoutConfig
void I2C_SDAStuckAtLowTimeoutConfig(I2C_TypeDef *I2Cx, uint32_t Timeout)
Configures the specified I2C SDA stuck at low timeout.
Definition: wb32f10x_i2c.c:141
I2C_DMARxReqLevelConfig
void I2C_DMARxReqLevelConfig(I2C_TypeDef *I2Cx, uint8_t Level)
Configures the DMA Rx request level.
Definition: wb32f10x_i2c.c:508
I2C_ReadData
uint16_t I2C_ReadData(I2C_TypeDef *I2Cx)
Read data from Rx FIFO.
Definition: wb32f10x_i2c.c:211
I2C_DMACmd
void I2C_DMACmd(I2C_TypeDef *I2Cx, uint32_t I2C_DMAReq, FunctionalState NewState)
Enables or disables the I2Cx's DMA interface.
Definition: wb32f10x_i2c.c:539
I2C_SMBus_GetRawITStatus
ITStatus I2C_SMBus_GetRawITStatus(I2C_TypeDef *I2Cx, uint16_t I2C_SMBUS_IT)
Checks whether the specified SMBus raw interrupt status.
Definition: wb32f10x_i2c.c:605