WB32F10x Standard Peripherals Firmware Library

Functions
LED_Private_Functions
WB32F10x_StdPeriph_Driver » LED

## Functions
void | LED_DeInit (void)
| Deinitializes the LED peripheral registers to their default reset values. More...
void | LED_Cmd (FunctionalState NewState)
| Enables or disables the LED peripheral. More...
void | LED_SetSegmentCode (uint8_t idx_seg, uint8_t seg_code)
| Set the segment code. More...
uint8_t | LED_GetSegmentCode (uint8_t idx_seg)
| Get the segment code. More...

## Detailed Description

## Function Documentation

## ◆ LED_Cmd()

void LED_Cmd | ( | FunctionalState | NewState | ) |

Enables or disables the LED peripheral.

Parameters

  NewState | new state of the LED peripheral. This parameter can be: ENABLE or DISABLE.

Returns
  None

## ◆ LED_DeInit()

void LED_DeInit | ( | void |  | ) |

Deinitializes the LED peripheral registers to their default reset values.

Returns
  None

## ◆ LED_GetSegmentCode()

uint8_t LED_GetSegmentCode | ( | uint8_t | idx_seg | ) |

Get the segment code.

Parameters

  idx_seg | The segment to set. This parameter must be between 0 to 7.

Returns
  The segment code.

## ◆ LED_SetSegmentCode()

void LED_SetSegmentCode | ( | uint8_t | idx_seg,
|  | uint8_t | seg_code
| ) |  |

Set the segment code.

Parameters

  idx_seg | The segment to set. This parameter must be between 0 to 7.
  seg_code | The segment code. This parameter must be between 0x00 to 0x7F.

Returns
  None