WB32F10x Standard Peripherals Firmware Library

Functions
wb32f10x_spi.c File Reference

This file provides all the SPI firmware functions. More...

`#include "wb32f10x_spi.h"`
`#include "wb32f10x_rcc.h"`

## Functions
void | SPI_DeInit (SPI_TypeDef *SPIx)
| Deinitializes the SPIx peripheral registers to their default reset values. More...
void | SPI_Init (SPI_TypeDef *SPIx, SPI_InitTypeDef *SPI_InitStruct)
| Initializes the SPIx peripheral according to the specified parameters in the SPI_InitStruct. More...
void | SPI_StructInit (SPI_InitTypeDef *SPI_InitStruct)
| Fills each SPI_InitStruct member with its default value. More...
void | SPI_Cmd (SPI_TypeDef *SPIx, FunctionalState NewState)
| Enables or disables the specified SPI peripheral. More...
void | SPI_TransferModeConfig (SPI_TypeDef *SPIx, uint16_t SPI_TransferMode)
| Configures the transfer mode. More...
void | SPI_SlaveOutputCmd (SPI_TypeDef *SPIx, FunctionalState NewState)
| Enables or disables the slave output (only used for SPISx). More...
void | SPI_NSSConfig (SPI_TypeDef *SPIx, uint32_t SPI_NSS, FunctionalState NewState)
| Enables or disables the specified slave select line (only used for SPIMx). More...
void | SPI_NSSToggleModeCmd (SPI_TypeDef *SPIx, FunctionalState NewState)
| Enables or disables the slave select toggle mode. More...
void | SPI_ReceiveDataLengthConfig (SPI_TypeDef *SPIx, uint32_t DataLength)
| Configures the number of data frames to be continuously received (only used for SPIMx). More...
void | SPI_MicrowireConfig (SPI_TypeDef *SPIx, SPI_MicrowireInitTypeDef *SPI_MicrowireInitStruct)
| Configures the Microwire frame format according to the specified parameters in the SPI_MicrowireInitStruct. More...
void | SPI_MicrowireStructInit (SPI_MicrowireInitTypeDef *SPI_MicrowireInitStruct)
| Fills each SPI_MicrowireInitStruct member with its default value. More...
void | SPI_SpiModeConfig (SPI_TypeDef *SPIx, uint32_t SPI_SpiMode)
| Configures the Spi Mode. More...
void | SPI_EnhancedSpiConfig (SPI_TypeDef *SPIx, SPI_EnhancedSpiInitTypeDef *SPI_EnhancedSpiInitStruct)
| Configures the Enhanced SPI Mode according to the specified parameters in the SPI_EnhancedSpiInitStruct (only used for QSPI). More...
void | SPI_EnhancedSpiStructInit (SPI_EnhancedSpiInitTypeDef *SPI_EnhancedSpiInitStruct)
| Fills each SPI_EnhancedSpiInitStruct member with its default value. More...
uint16_t | SPI_ReadData (SPI_TypeDef *SPIx)
| Read one data from Rx FIFO. More...
void | SPI_WriteData (SPI_TypeDef *SPIx, uint16_t Data)
| Write one data to Tx FIFO. More...
FlagStatus | SPI_GetFlagStatus (SPI_TypeDef *SPIx, uint8_t SPI_FLAG)
| Checks whether the specified SPIx flag is set or not. More...
void | SPI_ITConfig (SPI_TypeDef *SPIx, uint8_t SPI_IT, FunctionalState NewState)
| Enables or disables the specified SPI interrupts. More...
ITStatus | SPI_GetRawITStatus (SPI_TypeDef *SPIx, uint8_t SPI_IT)
| Checks whether the specified SPIx raw interrupt status. More...
ITStatus | SPI_GetITStatus (SPI_TypeDef *SPIx, uint8_t SPI_IT)
| Checks whether the specified SPIx interrupt has occurred or not. More...
void | SPI_ClearITPendingBit (SPI_TypeDef *SPIx, uint8_t SPI_IT)
| Clears the SPIx's interrupt pending bits. More...
void | SPI_RxFIFOThresholdConfig (SPI_TypeDef *SPIx, uint8_t Threshold)
| Configures the Rx FIFO threshold. More...
void | SPI_TxFIFOThresholdConfig (SPI_TypeDef *SPIx, uint8_t Threshold)
| Configures the Tx FIFO threshold. More...
uint8_t | SPI_GetRxFIFOLevel (SPI_TypeDef *SPIx)
| Returns the number of data can be read from Rx FIFO. More...
uint8_t | SPI_GetTxFIFOLevel (SPI_TypeDef *SPIx)
| Returns the number of data left in Tx FIFO. More...
void | SPI_DMARxReqLevelConfig (SPI_TypeDef *SPIx, uint8_t DMARxReqLevel)
| Configures the DMA Rx request level. More...
void | SPI_DMATxReqLevelConfig (SPI_TypeDef *SPIx, uint8_t DMATxReqLevel)
| Configures the DMA Tx request level. More...
void | SPI_DMACmd (SPI_TypeDef *SPIx, uint32_t SPI_DMAReq, FunctionalState NewState)
| Enables or disables the SPIx's DMA interface. More...
void | SPI_RxdSampleDelayConfig (SPI_TypeDef *SPIx, uint8_t DelayValue)
| Configures the rxd sample delay value. More...

## Detailed Description

This file provides all the SPI firmware functions.

Author
  Westberry Application Team

Version
  V0.1.10

Date
  05-January-2023