WB32F10x Standard Peripherals Firmware Library

Data Fields
RTC_TypeDef Struct Reference
CMSIS » Wb32f10x

## Data Fields
__IOM uint16_t | CRH
uint16_t | RESERVED0
__IOM uint16_t | CRL
uint16_t | RESERVED1
__OM uint16_t | PRLH
uint16_t | RESERVED2
union {
__IM uint32_t PRL
__OM uint16_t PRLL
}; |
__IM uint16_t | DIVH
uint16_t | RESERVED4
union {
__IM uint32_t DIV
__IM uint16_t DIVL
}; |
__IOM uint16_t | CNTH
uint16_t | RESERVED5
union {
__IM uint32_t CNT
__IOM uint16_t CNTL
}; |
__OM uint16_t | ALRH
uint16_t | RESERVED6
union {
__IM uint32_t ALR
__OM uint16_t ALRL
}; |

## Field Documentation

## ◆ ALR

__IM uint32_t ALR

RTC alarm register (read only), Address offset: 0x024

## ◆ ALRH

__OM uint16_t ALRH

RTC alarm register high, Address offset: 0x020

## ◆ ALRL

__OM uint16_t ALRL

RTC alarm register low, Address offset: 0x024

## ◆ CNT

__IM uint32_t CNT

RTC counter register (read only), Address offset: 0x01C

## ◆ CNTH

__IOM uint16_t CNTH

RTC counter register high, Address offset: 0x018

## ◆ CNTL

__IOM uint16_t CNTL

RTC counter register low, Address offset: 0x01C

## ◆ CRH

__IOM uint16_t CRH

RTC control register high, Address offset: 0x000

## ◆ CRL

__IOM uint16_t CRL

RTC control register low, Address offset: 0x004

## ◆ DIV

__IM uint32_t DIV

RTC prescaler divider register, Address offset: 0x014

## ◆ DIVH

__IM uint16_t DIVH

RTC prescaler divider register high, Address offset: 0x010

## ◆ DIVL

__IM uint16_t DIVL

RTC prescaler divider register low, Address offset: 0x014

## ◆ PRL

__IM uint32_t PRL

RTC prescaler load register (read only), Address offset: 0x00C

## ◆ PRLH

__OM uint16_t PRLH

RTC prescaler load register high, Address offset: 0x008

## ◆ PRLL

__OM uint16_t PRLL

RTC prescaler load register low, Address offset: 0x00C

The documentation for this struct was generated from the following file:

- wb32f10x.h