WB32F10x Standard Peripherals Firmware Library

函数
FMC_Private_Functions
WB32F10x_StdPeriph_Driver » FMC

## 函数
uint32_t | FMC_ClearPageLatch (void)
| Clear page latches. 更多...
uint32_t | FMC_ErasePage (uint32_t Page_Address)
| Erase a specified FLASH page. 更多...
uint32_t | FMC_EraseSector (uint32_t Sector_Address)
| Erase a specified FLASH sector. 更多...
uint32_t | FMC_EraseBulk (void)
| Erase main flash memory. 更多...
uint32_t | FMC_ProgramPage (uint32_t Page_Address)
| Programs the data to the specified page address. 更多...

## 详细描述

## 函数说明

## ◆ FMC_ClearPageLatch()

uint32_t FMC_ClearPageLatch | ( | void |  | ) |

Clear page latches.

返回
  0 - OK, 1 - Failed

注解
  Before calling this function, FHSI must be enabled.

## ◆ FMC_EraseBulk()

uint32_t FMC_EraseBulk | ( | void |  | ) |

Erase main flash memory.

返回
  0 - OK, 1 - Failed

注解
  Before calling this function, FHSI must be enabled.

## ◆ FMC_ErasePage()

uint32_t FMC_ErasePage | ( | uint32_t | Page_Address | ) |

Erase a specified FLASH page.

参数

  Page_Address | The page address to be erased.

返回
  0 - OK, 1 - Failed

注解
  Before calling this function, FHSI must be enabled.

## ◆ FMC_EraseSector()

uint32_t FMC_EraseSector | ( | uint32_t | Sector_Address | ) |

Erase a specified FLASH sector.

参数

  Sector_Address | The sector address to be erased.

返回
  0 - OK, 1 - Failed

注解
  Before calling this function, FHSI must be enabled.

## ◆ FMC_ProgramPage()

uint32_t FMC_ProgramPage | ( | uint32_t | Page_Address | ) |

Programs the data to the specified page address.

参数

  Page_Address | The page address to be programmed.

返回
  0 - OK, 1 - Failed

注解
  Before calling this function, FHSI must be enabled.