WB32F10x Standard Peripherals Firmware Library

Data Fields
TIM_ICInitTypeDef Struct Reference
WB32F10x_StdPeriph_Driver » TIM

TIM Input Capture Init structure definition. More...

`#include <wb32f10x_tim.h>`

## Data Fields
uint16_t | TIM_Channel
uint16_t | TIM_ICPolarity
uint16_t | TIM_ICSelection
uint16_t | TIM_ICPrescaler
uint16_t | TIM_ICFilter

## Detailed Description

TIM Input Capture Init structure definition.

## Field Documentation

## ◆ TIM_Channel

uint16_t TIM_Channel

Specifies the TIM channel. This parameter can be a value of TIM_Channel

## ◆ TIM_ICFilter

uint16_t TIM_ICFilter

Specifies the input capture filter. This parameter can be a number between 0x0 and 0xF

## ◆ TIM_ICPolarity

uint16_t TIM_ICPolarity

Specifies the active edge of the input signal. This parameter can be a value of TIM_Input_Capture_Polarity

## ◆ TIM_ICPrescaler

uint16_t TIM_ICPrescaler

Specifies the Input Capture Prescaler. This parameter can be a value of TIM_Input_Capture_Prescaler

## ◆ TIM_ICSelection

uint16_t TIM_ICSelection

Specifies the input. This parameter can be a value of TIM_Input_Capture_Selection

The documentation for this struct was generated from the following file:

- wb32f10x_tim.h