WB32F10x Standard Peripherals Firmware Library

成员变量
RCC_TypeDef结构体 参考
CMSIS » Wb32f10x

## 成员变量
__IOM uint32_t | PLLPRE
__IOM uint32_t | PLLSRC
__IOM uint32_t | MAINCLKSRC
__IOM uint32_t | MAINCLKUEN
uint32_t | RESERVED0
__IOM uint32_t | USBPRE
__IOM uint32_t | AHBPRE
__IOM uint32_t | APB1PRE
__IOM uint32_t | APB2PRE
__IOM uint32_t | MCLKPRE
__IOM uint32_t | I2SPRE
__IOM uint32_t | MCLKSRC
uint32_t | RESERVED1
__IOM uint32_t | USBFIFOCLKSRC
__IOM uint32_t | MCOSEL
__IOM uint32_t | AHBENR0
__IOM uint32_t | AHBENR1
__IOM uint32_t | AHBENR2
__IOM uint32_t | APB1ENR
__IOM uint32_t | APB2ENR
uint32_t | RESERVED2 [3]
__IOM uint32_t | RNGCLKENR
__IOM uint32_t | PCLKENR
__IOM uint32_t | IWDGCLKENR
uint32_t | RESERVED4
__IOM uint32_t | USBCLKENR
__IOM uint32_t | I2SCLKENR
__IOM uint32_t | SPIS1CLKENR
__IOM uint32_t | SPIS2CLKENR
__IOM uint32_t | USBFIFOCLKENR
uint32_t | RESERVED5 [2]
__IOM uint32_t | AHBRSTR1
uint32_t | RESERVED6
__IOM uint32_t | APB1RSTR
__IOM uint32_t | APB2RSTR
uint32_t | RESERVED7 [8]
__IOM uint32_t | I2SCLKRSTR
uint32_t | RESERVED8 [3]
__IOM uint32_t | CLRRSTSTAT
uint32_t | RESERVED9 [2]
__IOM uint32_t | BDRSTR
__IOM uint32_t | LSI2RTCENR
__IOM uint32_t | HSE2RTCENR
uint32_t | RESERVED10 [8]
__IOM uint32_t | RSTSTAT

## 结构体成员变量说明

## ◆ AHBENR0

__IOM uint32_t AHBENR0

RCC AHB peripheral clock enable register 0, Address offset: 0x03C

## ◆ AHBENR1

__IOM uint32_t AHBENR1

RCC AHB peripheral clock enable register 1, Address offset: 0x040

## ◆ AHBENR2

__IOM uint32_t AHBENR2

RCC AHB peripheral clock enable register 2, Address offset: 0x044

## ◆ AHBPRE

__IOM uint32_t AHBPRE

RCC AHB prescaler register, Address offset: 0x018

## ◆ AHBRSTR1

__IOM uint32_t AHBRSTR1

RCC AHB peripheral reset register 1, Address offset: 0x088

## ◆ APB1ENR

__IOM uint32_t APB1ENR

RCC APB1 peripheral clock enable register, Address offset: 0x048

## ◆ APB1PRE

__IOM uint32_t APB1PRE

RCC APB1 prescaler register, Address offset: 0x01C

## ◆ APB1RSTR

__IOM uint32_t APB1RSTR

RCC APB1 peripheral reset register, Address offset: 0x090

## ◆ APB2ENR

__IOM uint32_t APB2ENR

RCC APB2 peripheral clock enable register, Address offset: 0x04C

## ◆ APB2PRE

__IOM uint32_t APB2PRE

RCC APB2 prescaler register, Address offset: 0x020

## ◆ APB2RSTR

__IOM uint32_t APB2RSTR

RCC APB2 peripheral reset register, Address offset: 0x094

## ◆ BDRSTR

__IOM uint32_t BDRSTR

RCC Batt domain reset register, Address offset: 0x0D4

## ◆ CLRRSTSTAT

__IOM uint32_t CLRRSTSTAT

RCC clear reset status register, Address offset: 0x0C8

## ◆ HSE2RTCENR

__IOM uint32_t HSE2RTCENR

RCC HSE to RTC clock enable register, Address offset: 0x0DC

## ◆ I2SCLKENR

__IOM uint32_t I2SCLKENR

RCC I2S SCLK enable register, Address offset: 0x070

## ◆ I2SCLKRSTR

__IOM uint32_t I2SCLKRSTR

RCC I2S SCLK reset register, Address offset: 0x0B8

## ◆ I2SPRE

__IOM uint32_t I2SPRE

RCC I2S prescaler register, Address offset: 0x028

## ◆ IWDGCLKENR

__IOM uint32_t IWDGCLKENR

RCC IWDG clock enable register, Address offset: 0x064

## ◆ LSI2RTCENR

__IOM uint32_t LSI2RTCENR

RCC LSI to RTC clock enable register, Address offset: 0x0D8

## ◆ MAINCLKSRC

__IOM uint32_t MAINCLKSRC

RCC main clock source register, Address offset: 0x008

## ◆ MAINCLKUEN

__IOM uint32_t MAINCLKUEN

RCC main clock update enable register, Address offset: 0x00C

## ◆ MCLKPRE

__IOM uint32_t MCLKPRE

RCC MCLK prescaler register, Address offset: 0x024

## ◆ MCLKSRC

__IOM uint32_t MCLKSRC

RCC MCLK source register, Address offset: 0x02C

## ◆ MCOSEL

__IOM uint32_t MCOSEL

RCC MCO select register, Address offset: 0x038

## ◆ PCLKENR

__IOM uint32_t PCLKENR

RCC panel PCLK clock enable register, Address offset: 0x060

## ◆ PLLPRE

__IOM uint32_t PLLPRE

RCC PLL prescaler register, Address offset: 0x000

## ◆ PLLSRC

__IOM uint32_t PLLSRC

RCC PLL source register, Address offset: 0x004

## ◆ RESERVED0

uint32_t RESERVED0

Reserved, 0x010

## ◆ RESERVED1

uint32_t RESERVED1

Reserved, 0x030

## ◆ RESERVED10

uint32_t RESERVED10[8]

Reserved, 0x0E0 - 0x0FC

## ◆ RESERVED2

uint32_t RESERVED2[3]

Reserved, 0x050 - 0x058

## ◆ RESERVED4

uint32_t RESERVED4

Reserved, 0x068

## ◆ RESERVED5

uint32_t RESERVED5[2]

Reserved, 0x080 - 0x084

## ◆ RESERVED6

uint32_t RESERVED6

Reserved, 0x08C

## ◆ RESERVED7

uint32_t RESERVED7[8]

Reserved, 0x098 - 0x0B4

## ◆ RESERVED8

uint32_t RESERVED8[3]

Reserved, 0x0BC - 0x0C4

## ◆ RESERVED9

uint32_t RESERVED9[2]

Reserved, 0x0CC - 0x0D0

## ◆ RNGCLKENR

__IOM uint32_t RNGCLKENR

RCC RNG clock enable register, Address offset: 0x05C

## ◆ RSTSTAT

__IOM uint32_t RSTSTAT

RCC reset status register, Address offset: 0x100

## ◆ SPIS1CLKENR

__IOM uint32_t SPIS1CLKENR

RCC SPIS1 clock enable register, Address offset: 0x074

## ◆ SPIS2CLKENR

__IOM uint32_t SPIS2CLKENR

RCC SPIS2 clock enable register, Address offset: 0x078

## ◆ USBCLKENR

__IOM uint32_t USBCLKENR

RCC USB clock enable register, Address offset: 0x06C

## ◆ USBFIFOCLKENR

__IOM uint32_t USBFIFOCLKENR

RCC USB FIFO clock enable register, Address offset: 0x07C

## ◆ USBFIFOCLKSRC

__IOM uint32_t USBFIFOCLKSRC

RCC USB FIFO clock source register, Address offset: 0x034

## ◆ USBPRE

__IOM uint32_t USBPRE

RCC USB prescaler register, Address offset: 0x014

该结构体的文档由以下文件生成:

- wb32f10x.h