WB32F10x Standard Peripherals Firmware Library

Data Fields
RNG_TypeDef Struct Reference
CMSIS » Wb32f10x

## Data Fields
__IM uint32_t | RAND
__IOM uint32_t | STOP

## Field Documentation

## ◆ RAND

__IM uint32_t RAND

RNG generated 8bit random number register, Address offset: 0x000

## ◆ STOP

__IOM uint32_t STOP

RNG stop register, Address offset: 0x004

The documentation for this struct was generated from the following file:

- wb32f10x.h