WB32F10x Standard Peripherals Firmware Library

结构体
这里列出了所有结构体，并附带简要说明:

C__iar_u32 |
C_i2c_xfer_info_t |
C ADC_InitTypeDef | ADC Init structure definition
C ADC_TypeDef |
C AFIO_TypeDef |
C ANCTL_TypeDef |
C APSR_Type | Union type to access the Application Program Status Register (APSR)
C ARM_MPU_Region_t |
C BKP_TypeDef |
C CACHE_TypeDef |
C CONTROL_Type | Union type to access the Control Registers (CONTROL)
C CoreDebug_Type | Structure type to access the Core Debug Register (CoreDebug)
C CRC_TypeDef |
C DBGMCU_TypeDef |
C DMAC_Channel_InitTypeDef | DMAC Channel Init Structure definition
C DMAC_DestinationScatterInitTypeDef | DMAC Destination Scatter Structure definition
C DMAC_SourceGatherInitTypeDef | DMAC Source Gather Structure definition
C DMAC_TypeDef |
C DWT_Type | Structure type to access the Data Watchpoint and Trace Register (DWT)
C EXTI_InitTypeDef | EXTI Init Structure definition
C EXTI_TypeDef |
C FMC_TypeDef |
C GPIO_TypeDef |
C I2C_TypeDef |
C I2S_TypeDef |
C IPSR_Type | Union type to access the Interrupt Program Status Register (IPSR)
C ISO_TypeDef |
C ITM_Type | Structure type to access the Instrumentation Trace Macrocell Register (ITM)
C IWDG_TypeDef |
C LED_TypeDef |
C NVIC_InitTypeDef | NVIC Init Structure definition
C NVIC_Type | Structure type to access the Nested Vectored Interrupt Controller (NVIC)
C PWR_TypeDef |
C RCC_ClocksTypeDef |
C RCC_TypeDef |
C RNG_TypeDef |
C RTC_TypeDef |
C SCB_Type | Structure type to access the System Control Block (SCB)
C SCnSCB_Type | Structure type to access the System Control and ID Register not in the SCB
C SFM_TypeDef |
C SPI_EnhancedSpiInitTypeDef | SPI Enhanced SPI Mode Init structure definition
C SPI_InitTypeDef | SPI Init structure definition
C SPI_MicrowireInitTypeDef | SPI Microwire Init structure definition
C SPI_TypeDef |
C SYS_TypeDef |
C SysTick_Type | Structure type to access the System Timer (SysTick)
C TIM_BDTRInitTypeDef | BDTR structure definition
C TIM_ICInitTypeDef | TIM Input Capture Init structure definition
C TIM_OCInitTypeDef | TIM Output Compare Init structure definition
C TIM_TimeBaseInitTypeDef | TIM Time Base Init structure definition
C TIM_TypeDef |
C TPI_Type | Structure type to access the Trace Port Interface Register (TPI)
C UART_InitTypeDef | UART Init Structure definition
C UART_TypeDef |
C USB_TypeDef |
C usbd_msc_t |
C UsbdCoreInfo_t |
C WWDG_TypeDef |
C xPSR_Type | Union type to access the Special-Purpose Program Status Registers (xPSR)