WB32F10x Standard Peripherals Firmware Library

宏定义
EXTI_Lines
WB32F10x_StdPeriph_Driver » EXTI » EXTI_Exported_Constants

## 宏定义
#define | EXTI_Line0 ((uint32_t)0x00001)
#define | EXTI_Line1 ((uint32_t)0x00002)
#define | EXTI_Line2 ((uint32_t)0x00004)
#define | EXTI_Line3 ((uint32_t)0x00008)
#define | EXTI_Line4 ((uint32_t)0x00010)
#define | EXTI_Line5 ((uint32_t)0x00020)
#define | EXTI_Line6 ((uint32_t)0x00040)
#define | EXTI_Line7 ((uint32_t)0x00080)
#define | EXTI_Line8 ((uint32_t)0x00100)
#define | EXTI_Line9 ((uint32_t)0x00200)
#define | EXTI_Line10 ((uint32_t)0x00400)
#define | EXTI_Line11 ((uint32_t)0x00800)
#define | EXTI_Line12 ((uint32_t)0x01000)
#define | EXTI_Line13 ((uint32_t)0x02000)
#define | EXTI_Line14 ((uint32_t)0x04000)
#define | EXTI_Line15 ((uint32_t)0x08000)
#define | EXTI_Line16 ((uint32_t)0x10000)
#define | EXTI_Line17 ((uint32_t)0x20000)
#define | EXTI_Line18 ((uint32_t)0x40000)
#define | IS_EXTI_LINE(LINE) ((((LINE) & (uint32_t)0xFFF00000) == 0x00) && ((LINE) != (uint16_t)0x00))
#define | IS_GET_EXTI_LINE(LINE)

## 详细描述

## 宏定义说明

## ◆ EXTI_Line0

#define EXTI_Line0 ((uint32_t)0x00001)

External interrupt line 0

## ◆ EXTI_Line1

#define EXTI_Line1 ((uint32_t)0x00002)

External interrupt line 1

## ◆ EXTI_Line10

#define EXTI_Line10 ((uint32_t)0x00400)

External interrupt line 10

## ◆ EXTI_Line11

#define EXTI_Line11 ((uint32_t)0x00800)

External interrupt line 11

## ◆ EXTI_Line12

#define EXTI_Line12 ((uint32_t)0x01000)

External interrupt line 12

## ◆ EXTI_Line13

#define EXTI_Line13 ((uint32_t)0x02000)

External interrupt line 13

## ◆ EXTI_Line14

#define EXTI_Line14 ((uint32_t)0x04000)

External interrupt line 14

## ◆ EXTI_Line15

#define EXTI_Line15 ((uint32_t)0x08000)

External interrupt line 15

## ◆ EXTI_Line16

#define EXTI_Line16 ((uint32_t)0x10000)

External interrupt line 16 Connected to the PVD Output

## ◆ EXTI_Line17

#define EXTI_Line17 ((uint32_t)0x20000)

External interrupt line 17 Connected to the RTC Alarm event

## ◆ EXTI_Line18

#define EXTI_Line18 ((uint32_t)0x40000)

External interrupt line 18 Connected to the USB Wakeup event

## ◆ EXTI_Line2

#define EXTI_Line2 ((uint32_t)0x00004)

External interrupt line 2

## ◆ EXTI_Line3

#define EXTI_Line3 ((uint32_t)0x00008)

External interrupt line 3

## ◆ EXTI_Line4

#define EXTI_Line4 ((uint32_t)0x00010)

External interrupt line 4

## ◆ EXTI_Line5

#define EXTI_Line5 ((uint32_t)0x00020)

External interrupt line 5

## ◆ EXTI_Line6

#define EXTI_Line6 ((uint32_t)0x00040)

External interrupt line 6

## ◆ EXTI_Line7

#define EXTI_Line7 ((uint32_t)0x00080)

External interrupt line 7

## ◆ EXTI_Line8

#define EXTI_Line8 ((uint32_t)0x00100)

External interrupt line 8

## ◆ EXTI_Line9

#define EXTI_Line9 ((uint32_t)0x00200)

External interrupt line 9

## ◆ IS_GET_EXTI_LINE

#define IS_GET_EXTI_LINE | ( |  | LINE | ) |

值:
(((LINE) == EXTI_Line0) || ((LINE) == EXTI_Line1) || \
((LINE) == EXTI_Line2) || ((LINE) == EXTI_Line3) || \
((LINE) == EXTI_Line4) || ((LINE) == EXTI_Line5) || \
((LINE) == EXTI_Line6) || ((LINE) == EXTI_Line7) || \
((LINE) == EXTI_Line8) || ((LINE) == EXTI_Line9) || \
((LINE) == EXTI_Line10) || ((LINE) == EXTI_Line11) || \
((LINE) == EXTI_Line12) || ((LINE) == EXTI_Line13) || \
((LINE) == EXTI_Line14) || ((LINE) == EXTI_Line15) || \
((LINE) == EXTI_Line16) || ((LINE) == EXTI_Line17) || \
((LINE) == EXTI_Line18))
EXTI_Line1
#define EXTI_Line1
Definition: wb32f10x_exti.h:85
EXTI_Line13
#define EXTI_Line13
Definition: wb32f10x_exti.h:97
EXTI_Line17
#define EXTI_Line17
Definition: wb32f10x_exti.h:101
EXTI_Line2
#define EXTI_Line2
Definition: wb32f10x_exti.h:86
EXTI_Line16
#define EXTI_Line16
Definition: wb32f10x_exti.h:100
EXTI_Line10
#define EXTI_Line10
Definition: wb32f10x_exti.h:94
EXTI_Line11
#define EXTI_Line11
Definition: wb32f10x_exti.h:95
EXTI_Line14
#define EXTI_Line14
Definition: wb32f10x_exti.h:98
EXTI_Line12
#define EXTI_Line12
Definition: wb32f10x_exti.h:96
EXTI_Line7
#define EXTI_Line7
Definition: wb32f10x_exti.h:91
EXTI_Line18
#define EXTI_Line18
Definition: wb32f10x_exti.h:102
EXTI_Line5
#define EXTI_Line5
Definition: wb32f10x_exti.h:89
EXTI_Line0
#define EXTI_Line0
Definition: wb32f10x_exti.h:84
EXTI_Line15
#define EXTI_Line15
Definition: wb32f10x_exti.h:99
EXTI_Line3
#define EXTI_Line3
Definition: wb32f10x_exti.h:87
EXTI_Line9
#define EXTI_Line9
Definition: wb32f10x_exti.h:93
EXTI_Line6
#define EXTI_Line6
Definition: wb32f10x_exti.h:90
EXTI_Line4
#define EXTI_Line4
Definition: wb32f10x_exti.h:88
EXTI_Line8
#define EXTI_Line8
Definition: wb32f10x_exti.h:92