WB32F10x Standard Peripherals Firmware Library

Macros | Functions
wb32f10x_wwdg.h File Reference

This file contains all the functions prototypes for the WWDG firmware library. More...

`#include "wb32f10x.h"`

Go to the source code of this file.

## Macros
#define | WWDG_Prescaler_1 ((uint32_t)0x00000000)
#define | WWDG_Prescaler_2 ((uint32_t)0x00000080)
#define | WWDG_Prescaler_4 ((uint32_t)0x00000100)
#define | WWDG_Prescaler_8 ((uint32_t)0x00000180)
#define | IS_WWDG_PRESCALER(PRESCALER)
#define | IS_WWDG_WINDOW_VALUE(VALUE) ((VALUE) <= 0x7F)
#define | IS_WWDG_COUNTER(COUNTER) (((COUNTER) >= 0x40) && ((COUNTER) <= 0x7F))

## Functions
void | WWDG_DeInit (void)
| Deinitializes the WWDG peripheral registers to their default reset values. More...
void | WWDG_SetPrescaler (uint32_t WWDG_Prescaler)
| Sets the WWDG Prescaler. More...
void | WWDG_SetWindowValue (uint8_t WindowValue)
| Sets the WWDG window value. More...
void | WWDG_EnableIT (void)
| Enables the WWDG Early Wakeup interrupt(EWI). More...
void | WWDG_SetCounter (uint8_t Counter)
| Sets the WWDG counter value. More...
void | WWDG_Enable (uint8_t Counter)
| Enables WWDG and load the counter value. More...
FlagStatus | WWDG_GetFlagStatus (void)
| Checks whether the Early Wakeup interrupt flag is set or not. More...
void | WWDG_ClearFlag (void)
| Clears Early Wakeup interrupt flag. More...

## Detailed Description

This file contains all the functions prototypes for the WWDG firmware library.

Author
  Westberry Application Team

Version
  V0.1.10

Date
  05-January-2023