WB32F10x Standard Peripherals Firmware Library

结构体 | 宏定义
Instrumentation Trace Macrocell (ITM)
Defines and Type Definitions

Type definitions for the Instrumentation Trace Macrocell (ITM) 更多...

## 结构体
struct | ITM_Type
| Structure type to access the Instrumentation Trace Macrocell Register (ITM). 更多...

## 宏定义
#define | ITM_TPR_PRIVMASK_Pos 0U
#define | ITM_TPR_PRIVMASK_Msk (0xFFFFFFFFUL /*<< ITM_TPR_PRIVMASK_Pos*/)
#define | ITM_TCR_BUSY_Pos 23U
#define | ITM_TCR_BUSY_Msk (1UL << ITM_TCR_BUSY_Pos)
#define | ITM_TCR_TraceBusID_Pos 16U
#define | ITM_TCR_TraceBusID_Msk (0x7FUL << ITM_TCR_TraceBusID_Pos)
#define | ITM_TCR_GTSFREQ_Pos 10U
#define | ITM_TCR_GTSFREQ_Msk (3UL << ITM_TCR_GTSFREQ_Pos)
#define | ITM_TCR_TSPrescale_Pos 8U
#define | ITM_TCR_TSPrescale_Msk (3UL << ITM_TCR_TSPrescale_Pos)
#define | ITM_TCR_SWOENA_Pos 4U
#define | ITM_TCR_SWOENA_Msk (1UL << ITM_TCR_SWOENA_Pos)
#define | ITM_TCR_DWTENA_Pos 3U
#define | ITM_TCR_DWTENA_Msk (1UL << ITM_TCR_DWTENA_Pos)
#define | ITM_TCR_SYNCENA_Pos 2U
#define | ITM_TCR_SYNCENA_Msk (1UL << ITM_TCR_SYNCENA_Pos)
#define | ITM_TCR_TSENA_Pos 1U
#define | ITM_TCR_TSENA_Msk (1UL << ITM_TCR_TSENA_Pos)
#define | ITM_TCR_ITMENA_Pos 0U
#define | ITM_TCR_ITMENA_Msk (1UL /*<< ITM_TCR_ITMENA_Pos*/)
#define | ITM_IWR_ATVALIDM_Pos 0U
#define | ITM_IWR_ATVALIDM_Msk (1UL /*<< ITM_IWR_ATVALIDM_Pos*/)
#define | ITM_IRR_ATREADYM_Pos 0U
#define | ITM_IRR_ATREADYM_Msk (1UL /*<< ITM_IRR_ATREADYM_Pos*/)
#define | ITM_IMCR_INTEGRATION_Pos 0U
#define | ITM_IMCR_INTEGRATION_Msk (1UL /*<< ITM_IMCR_INTEGRATION_Pos*/)
#define | ITM_LSR_ByteAcc_Pos 2U
#define | ITM_LSR_ByteAcc_Msk (1UL << ITM_LSR_ByteAcc_Pos)
#define | ITM_LSR_Access_Pos 1U
#define | ITM_LSR_Access_Msk (1UL << ITM_LSR_Access_Pos)
#define | ITM_LSR_Present_Pos 0U
#define | ITM_LSR_Present_Msk (1UL /*<< ITM_LSR_Present_Pos*/)

## 详细描述

Type definitions for the Instrumentation Trace Macrocell (ITM)

## 宏定义说明

## ◆ ITM_IMCR_INTEGRATION_Msk

#define ITM_IMCR_INTEGRATION_Msk (1UL /*<< ITM_IMCR_INTEGRATION_Pos*/)

ITM IMCR: INTEGRATION Mask

## ◆ ITM_IMCR_INTEGRATION_Pos

#define ITM_IMCR_INTEGRATION_Pos 0U

ITM IMCR: INTEGRATION Position

## ◆ ITM_IRR_ATREADYM_Msk

#define ITM_IRR_ATREADYM_Msk (1UL /*<< ITM_IRR_ATREADYM_Pos*/)

ITM IRR: ATREADYM Mask

## ◆ ITM_IRR_ATREADYM_Pos

#define ITM_IRR_ATREADYM_Pos 0U

ITM IRR: ATREADYM Position

## ◆ ITM_IWR_ATVALIDM_Msk

#define ITM_IWR_ATVALIDM_Msk (1UL /*<< ITM_IWR_ATVALIDM_Pos*/)

ITM IWR: ATVALIDM Mask

## ◆ ITM_IWR_ATVALIDM_Pos

#define ITM_IWR_ATVALIDM_Pos 0U

ITM IWR: ATVALIDM Position

## ◆ ITM_LSR_Access_Msk

#define ITM_LSR_Access_Msk (1UL << ITM_LSR_Access_Pos)

ITM LSR: Access Mask

## ◆ ITM_LSR_Access_Pos

#define ITM_LSR_Access_Pos 1U

ITM LSR: Access Position

## ◆ ITM_LSR_ByteAcc_Msk

#define ITM_LSR_ByteAcc_Msk (1UL << ITM_LSR_ByteAcc_Pos)

ITM LSR: ByteAcc Mask

## ◆ ITM_LSR_ByteAcc_Pos

#define ITM_LSR_ByteAcc_Pos 2U

ITM LSR: ByteAcc Position

## ◆ ITM_LSR_Present_Msk

#define ITM_LSR_Present_Msk (1UL /*<< ITM_LSR_Present_Pos*/)

ITM LSR: Present Mask

## ◆ ITM_LSR_Present_Pos

#define ITM_LSR_Present_Pos 0U

ITM LSR: Present Position

## ◆ ITM_TCR_BUSY_Msk

#define ITM_TCR_BUSY_Msk (1UL << ITM_TCR_BUSY_Pos)

ITM TCR: BUSY Mask

## ◆ ITM_TCR_BUSY_Pos

#define ITM_TCR_BUSY_Pos 23U

ITM TCR: BUSY Position

## ◆ ITM_TCR_DWTENA_Msk

#define ITM_TCR_DWTENA_Msk (1UL << ITM_TCR_DWTENA_Pos)

ITM TCR: DWTENA Mask

## ◆ ITM_TCR_DWTENA_Pos

#define ITM_TCR_DWTENA_Pos 3U

ITM TCR: DWTENA Position

## ◆ ITM_TCR_GTSFREQ_Msk

#define ITM_TCR_GTSFREQ_Msk (3UL << ITM_TCR_GTSFREQ_Pos)

ITM TCR: Global timestamp frequency Mask

## ◆ ITM_TCR_GTSFREQ_Pos

#define ITM_TCR_GTSFREQ_Pos 10U

ITM TCR: Global timestamp frequency Position

## ◆ ITM_TCR_ITMENA_Msk

#define ITM_TCR_ITMENA_Msk (1UL /*<< ITM_TCR_ITMENA_Pos*/)

ITM TCR: ITM Enable bit Mask

## ◆ ITM_TCR_ITMENA_Pos

#define ITM_TCR_ITMENA_Pos 0U

ITM TCR: ITM Enable bit Position

## ◆ ITM_TCR_SWOENA_Msk

#define ITM_TCR_SWOENA_Msk (1UL << ITM_TCR_SWOENA_Pos)

ITM TCR: SWOENA Mask

## ◆ ITM_TCR_SWOENA_Pos

#define ITM_TCR_SWOENA_Pos 4U

ITM TCR: SWOENA Position

## ◆ ITM_TCR_SYNCENA_Msk

#define ITM_TCR_SYNCENA_Msk (1UL << ITM_TCR_SYNCENA_Pos)

ITM TCR: SYNCENA Mask

## ◆ ITM_TCR_SYNCENA_Pos

#define ITM_TCR_SYNCENA_Pos 2U

ITM TCR: SYNCENA Position

## ◆ ITM_TCR_TraceBusID_Msk

#define ITM_TCR_TraceBusID_Msk (0x7FUL << ITM_TCR_TraceBusID_Pos)

ITM TCR: ATBID Mask

## ◆ ITM_TCR_TraceBusID_Pos

#define ITM_TCR_TraceBusID_Pos 16U

ITM TCR: ATBID Position

## ◆ ITM_TCR_TSENA_Msk

#define ITM_TCR_TSENA_Msk (1UL << ITM_TCR_TSENA_Pos)

ITM TCR: TSENA Mask

## ◆ ITM_TCR_TSENA_Pos

#define ITM_TCR_TSENA_Pos 1U

ITM TCR: TSENA Position

## ◆ ITM_TCR_TSPrescale_Msk

#define ITM_TCR_TSPrescale_Msk (3UL << ITM_TCR_TSPrescale_Pos)

ITM TCR: TSPrescale Mask

## ◆ ITM_TCR_TSPrescale_Pos

#define ITM_TCR_TSPrescale_Pos 8U

ITM TCR: TSPrescale Position

## ◆ ITM_TPR_PRIVMASK_Msk

#define ITM_TPR_PRIVMASK_Msk (0xFFFFFFFFUL /*<< ITM_TPR_PRIVMASK_Pos*/)

ITM TPR: PRIVMASK Mask

## ◆ ITM_TPR_PRIVMASK_Pos

#define ITM_TPR_PRIVMASK_Pos 0U

ITM TPR: PRIVMASK Position