WB32F10x Standard Peripherals Firmware Library

Macros
PLL_entry_clock_source
WB32F10x_StdPeriph_Driver » RCC » RCC_Exported_Constants

## Macros
#define | RCC_PLLSource_HSE_Div1 ((uint32_t)0x00000100)
#define | RCC_PLLSource_HSE_Div2 ((uint32_t)0x00000101)
#define | RCC_PLLSource_HSE_Div3 ((uint32_t)0x00000103)
#define | RCC_PLLSource_HSE_Div4 ((uint32_t)0x00000105)
#define | RCC_PLLSource_HSE_Div5 ((uint32_t)0x00000107)
#define | RCC_PLLSource_HSE_Div6 ((uint32_t)0x00000109)
#define | RCC_PLLSource_HSE_Div7 ((uint32_t)0x0000010B)
#define | RCC_PLLSource_HSE_Div8 ((uint32_t)0x0000010D)
#define | RCC_PLLSource_HSE_Div9 ((uint32_t)0x0000010F)
#define | RCC_PLLSource_HSE_Div10 ((uint32_t)0x00000111)
#define | RCC_PLLSource_HSE_Div11 ((uint32_t)0x00000113)
#define | RCC_PLLSource_HSE_Div12 ((uint32_t)0x00000115)
#define | RCC_PLLSource_HSE_Div13 ((uint32_t)0x00000117)
#define | RCC_PLLSource_HSE_Div14 ((uint32_t)0x00000119)
#define | RCC_PLLSource_HSE_Div15 ((uint32_t)0x0000011B)
#define | RCC_PLLSource_HSE_Div16 ((uint32_t)0x0000011D)
#define | RCC_PLLSource_MHSI_Div1 ((uint32_t)0x00000000)
#define | RCC_PLLSource_MHSI_Div2 ((uint32_t)0x00000001)
#define | RCC_PLLSource_MHSI_Div3 ((uint32_t)0x00000003)
#define | RCC_PLLSource_MHSI_Div4 ((uint32_t)0x00000005)
#define | RCC_PLLSource_MHSI_Div5 ((uint32_t)0x00000007)
#define | RCC_PLLSource_MHSI_Div6 ((uint32_t)0x00000009)
#define | RCC_PLLSource_MHSI_Div7 ((uint32_t)0x0000000B)
#define | RCC_PLLSource_MHSI_Div8 ((uint32_t)0x0000000D)
#define | RCC_PLLSource_MHSI_Div9 ((uint32_t)0x0000000F)
#define | RCC_PLLSource_MHSI_Div10 ((uint32_t)0x00000011)
#define | RCC_PLLSource_MHSI_Div11 ((uint32_t)0x00000013)
#define | RCC_PLLSource_MHSI_Div12 ((uint32_t)0x00000015)
#define | RCC_PLLSource_MHSI_Div13 ((uint32_t)0x00000017)
#define | RCC_PLLSource_MHSI_Div14 ((uint32_t)0x00000019)
#define | RCC_PLLSource_MHSI_Div15 ((uint32_t)0x0000001B)
#define | RCC_PLLSource_MHSI_Div16 ((uint32_t)0x0000001D)

## Detailed Description